{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":12,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FBQ100C8VEB / RZQSG100L8Y1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQSG100L8Y1B","FBQ50C8VEB / FBQ50C8VEB / RZQSG100L8Y1B","FBQ125C8VEB / RZQSG125L8Y1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQSG125L8Y1B","FBQ50C8VEB / FBQ50C8VEB / FBQ50C8VEB / RZQSG125L8Y1B","FBQ60C8VEB / FBQ60C8VEB / RZQSG125L8Y1B","FBQ140C8VEB / RZQSG140L7Y1B"]
["Капацитет на охлаждане","Ном.","","кВт","9.5","","","12.0","","","","13.4"]
["Охлаждане с конвекция","SEER","","","5.5","5.1","5.1","5.2","4.8","4.8","4.8"]
["","Годишно потребление на електроенергия","","kWh/a","605","652","652","808","875","875","875"]
["","Капацитет","Pdesign","кВт","9.5","9.5","9.5","12","12","12","12"]
["","Клас на енергийна ефективност","","","A","B","B","A","B","B","B"]
["Отопление с конвекция (умерен климат)","Капацитет","Pdesign","кВт","7.6","7.6","7.6","7.6","7.6","7.6","7.6"]
["","SCOP/A","","","4.01","3.8","3.8","3.9","3.8","3.8","3.8"]
["","Клас на енергийна ефективност","","","A+","A","A","A","A","A","A"]
["","Годишно потребление на електроенергия","","kWh/a","2,654","2,800","2,800","2,729","2,800","2,800","2,800"]
["Номинална ефективност","Годишен разход на енергия","","kWh","1,435","","","1,870","","","","2,220"]
["","EER","","","3.31","","","3.21","","","","3.02"]
["","COP","","","3.65","","","3.51","","","","3.41"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","A","","","A"]
["","","Отопление","","A","","","B"]
["Топлинен капацитет","Ном.","","кВт","10.8","","","13.5","","","","15.5"]
["Забележки","","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС"]
["","","","","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване","","","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване","","","","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване"]
["","","","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС"]