{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":13,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FBQ35D2VEB / FBQ35D2VEB / RZQSG71L3V1B","FBQ100D2VEB / RZQSG100L9V1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQSG100L9V1B","FBQ50D2VEB / FBQ50D2VEB / RZQSG100L9V1B","FBQ125D2VEB / RZQSG125L9V1B","FBQ50D2VEB / FBQ50D2VEB / FBQ50D2VEB / RZQSG125L9V1B","FBQ60D2VEB / FBQ60D2VEB / RZQSG125L9V1B","FBQ140D2VEB / RZQSG140L9V1B","FBQ71D2VEB / RZQSG71L3V1B (Archived)"]
["Охлаждане с конвекция","SEER","","","5.10","5.61","5.10","5.10","5.47","4.80","4.80"]
["","Годишно потребление на електроенергия","","kWh/a","467","593","652","652","768","875","875"]
["","Капацитет","Pdesign","кВт","6.80","9.50","9.50","9.50","12.00","12.00","12.00"]
["","Клас на енергийна ефективност","","","A","A+","A","A","A","B","B"]
["Отопление с конвекция (умерен климат)","Капацитет","Pdesign","кВт","6.00","7.60","7.60","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","3.80","4.15","3.80","3.80","4.01","3.80","3.80"]
["","Клас на енергийна ефективност","","","A","A+","A","A","A+","A","A"]
["","Годишно потребление на електроенергия","","kWh/a","2,211","2,564","2,800","2,800","2,653","2,800","2,800"]
["Забележки","","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС"]
["","","","","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване","","","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване","","","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване"]
["Капацитет на охлаждане","Ном.","","кВт","","9.5 (2)","","","12.0 (2)","","","13.4 (2)"]
["Номинална ефективност","Годишен разход на енергия","","kWh","","1,418","","","1,858"]
["","EER","","","","3.35 (1)","","","3.23 (1)","","","3.06 (1)"]
["","COP","","","","3.67 (1)","","","3.63 (1)","","","3.40 (1)"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","","A","","","A"]
["","","Отопление","","","A","","","A"]
["Капацитет на отопление","Ном.","","кВт","","10.80 (2)","","","13.50 (2)","","","15.50 (2)"]
["Забележки","","","","","(3) - Годишният разход на електроенергия е съгласно Директивата за енергиен клас 2002/31/EC","","","(3) - Годишният разход на електроенергия е съгласно Директивата за енергиен клас 2002/31/EC"]
["","","","","","(4) - SEER и SCOP са съгласно EN 14825","","","(4) - SEER и SCOP са съгласно EN 14825"]
["","","","","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС"]
["Външно тяло","","","","","","","","","","","","RZQSG71L3V1"]
["Капацитет на охлаждане","Ном.","","кВт","","","","","","","","","6.8"]
["Топлинен капацитет","Ном.","","кВт","","","","","","","","","7.5"]
["Номинална ефективност","EER","","","","","","","","","","","3.30"]
["","COP","","","","","","","","","","","3.81"]
["","Годишен разход на енергия","","kWh","","","","","","","","","1030"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","","","","","","","","","A"]
["","","Отопление","","","","","","","","","","A"]
["Охлаждане с конвекция","Клас на енергийна ефективност","","","","","","","","","","","A+"]
["","Капацитет","Pdesign","кВт","","","","","","","","","6.80"]
["","SEER","","","","","","","","","","","5.84"]
["","Годишно потребление на електроенергия","","kWh/a","","","","","","","","","408"]
["Отопление с конвекция (умерен климат)","Клас на енергийна ефективност","","","","","","","","","","","A+"]
["","Капацитет","Pdesign","кВт","","","","","","","","","6.00"]
["","SCOP/A","","","","","","","","","","","4.10"]
["","Годишно потребление на електроенергия","","kWh/a","","","","","","","","","2049"]