{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":5,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RXS-L3"]
[]
[]
[]
[]
["","","","","FCAG35AVEB / RXS35L3V1B"]
["Капацитет на охлаждане","Ном.","","кВт","3.40"]
["Охлаждане с конвекция","SEER","","","6.35"]
["","Годишно потребление на електроенергия","","kWh/a","193"]
["","Капацитет","Pdesign","кВт","3.50"]
["","Клас на енергийна ефективност","","","A++"]
["Отопление с конвекция (умерен климат)","Капацитет","Pdesign","кВт","3.32"]
["","SCOP/A","","","4.90"]
["","Клас на енергийна ефективност","","","A++"]
["","Годишно потребление на електроенергия","","kWh/a","949"]
["Тръбни съединения","Tечност","Вън. д.","мм","6.35"]
["","Газ","Вън. д.","мм","9.50"]
["","Дренаж","вън. д.","мм","VP25 (Външен диам. 32, вътр. диам. 25)"]
["Номинална ефективност","EER","","","3.74"]
["","Годишен разход на енергия","","kWh","455"]
["","COP","","","3.50"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","A"]
["","","Отопление","","B"]
["Капацитет на отопление","Ном.","","кВт","4.20"]
["Забележки","","","","(1) - Номиналният капацитет на охлаждане се базира на: вътрешна температура: 27°CDB, 19°CWB, външна температура: 35°CDB, еквивалентна дължина на тръбите за хладилен агент: 5 m, разлика в нивото: 0m."]
["","","","","(2) - Номиналният капацитет за загряване важи за: вътрешна температура: 20°C (сух термометър), външна температура: 7°C (сух термометър), 8°C (влажен термометър), съответна дължина на тръбите: 5 м, денивелация: 0m."]
["","","","","(3) - Вж. отделния чертеж за работен диапазон"]
["","","","","(4) - Вж. отделния чертеж за електрическите схеми"]