{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":13,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100GVEB / RZQG100L8Y1B","FCAHG125GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG100L8Y1B","FCAHG140GVEB / RZQG125L8Y1B","FCAHG100GVEB / RZQG71L8Y1B","FCAHG71GVEB / RZQG71L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG100L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG140L7Y1B"]
["Капацитет на охлаждане","Ном.","","кВт","","","","","","6.80 (1)","","","13.4 (1)"]
["Охлаждане с конвекция","SEER","","","","","","","6.91","6.91","","","6.75"]
["","ηs,c","","%","","","","","","","","","266.9"]
["","Годишно потребление на електроенергия","","kWh/a","","","","","345","345","","","1,191"]
["","Капацитет","Pdesign","кВт","","","","","6.80","6.80","","","13.4"]
["","Клас на енергийна ефективност","","","","","","","A++","A++"]
["Отопление с конвекция (умерен климат)","Капацитет","Pdesign","кВт","","","","","7.60","7.60","","","11.8"]
["","SCOP/A","","","","","","","4.54","4.54","","","4.38"]
["","Клас на енергийна ефективност","","","","","","","A+","A+"]
["","Годишно потребление на електроенергия","","kWh/a","","","","","2,344","2,344","","","3,766"]
["","ηs,h","","%","","","","","","","","","172.1"]
["Номинална ефективност","Годишен разход на енергия","","kWh","","","","","","830"]
["","EER","","","","","","","","4.09 (3)","","","3.18 (3)"]
["","COP","","","","","","","","4.80 (3)","","","4.12 (3)"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","","","","","","A"]
["","","Отопление","","","","","","","A"]
["Капацитет на отопление","Ном.","","кВт","","","","","","7.50 (2)","","","15.5 (2)"]
["Диапазон на енергийна ефективност","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","A+++ ~ D","A+++ ~ D"]
["Забележки","","","","","","","","","(1) - Охлаждане: температура на открито 27°C (сух термометър), 19°C (влажен термометър); външна температура 35°C със сух термометър; дължина на еквивал. тръбопр.: 7,5 м; денивелация: 0 м.","","","(1) - Охлаждане: температура на открито 27°C (сух термометър), 19°C (влажен термометър); външна температура 35°C със сух термометър; дължина на еквивал. тръбопр.: 7,5 м; денивелация: 0 м."]
["","","","","","","","","","(2) - Отопление: температура на открито 20°С (сух термометър), външна темп. 7°C (сух термометър), 6°C (влажен термометър); съответна дължина на тръбите за хладилния агент: 7,5 м; денивелация: 0 м.","","","(2) - Отопление: температура на открито 20°С (сух термометър), външна темп. 7°C (сух термометър), 6°C (влажен термометър); съответна дължина на тръбите за хладилния агент: 7,5 м; денивелация: 0 м."]
["","","","","","","","","","(3) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","","","(3) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС"]
["Външно тяло","","","","","","","","","","RZQG100L8Y1","RZQG125L8Y1"]
["Охлаждане с конвекция","Клас на енергийна ефективност","","","","","","","","","A","A"]
["","Капацитет","Pdesign","кВт","","","","","","","9.50","12.0"]
["","SEER","","","","","","","","","5.10","5.10"]
["","Годишно потребление на електроенергия","","kWh/a","","","","","","","652","824"]
["Отопление с конвекция (умерен климат)","Клас на енергийна ефективност","","","","","","","","","A","A"]
["","Капацитет","Pdesign","кВт","","","","","","","11.30","12.71"]
["","SCOP/A","","","","","","","","","3.80","3.80"]
["","Pdh Капацитет на отопление при -10°","","кВт","","","","","","","9.66","11.4"]
["","Годишно потребление на електроенергия","","kWh/a","","","","","","","4164","4683"]