{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQ-C8 / RXS-F"]
[]
[]
[]
[]
["","","","","FCQ60C8VEB / RXS60F3V1B"]
["Капацитет на охлаждане","Мин.","","кВт","0.9"]
["","Макс.","","кВт","6.0"]
["","Ном.","","кВт","5.7 (1)"]
["Тръбни съединения","Tечност","Вън. д.","мм","6.35"]
["","Газ","Вън. д.","мм","12.7"]
["","Дренаж","вън. д.","мм","32"]
["Номинална ефективност","Годишен разход на енергия","","kWh","820"]
["","EER","","","3.48"]
["","COP","","","3.52"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","A"]
["","","Отопление","","B"]
["Капацитет на отопление","Ном.","","кВт","7.0 (2)"]
["","Мин.","","кВт","0.9"]
["","Макс.","","кВт","8.0"]
["Забележки","","","","(1) - Охлаждане: температура на открито 27°C със сух термометър, 19.0°C с влажен термометър; външна темп. 35°C със сух термометър; дължина на еквивал. тръбопр.: 5м"]
["","","","","(2) - Отопление: температура на открито 20°С (сух термометър), външна темп. 7°C (сух термометър), 6°C (влажен термометър); съответна дължина на тръбите за хладилния агент: 5м"]
["","","","","(3) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване"]