{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":11,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCQHG100FVEB / RZQG71L8Y1B","FCQHG71FVEB / RZQG71L8Y1B","FCQHG140FVEB / RZQG100L8Y1B","FCQHG71FVEB / FCQHG71FVEB / RZQG100L8Y1B","FCQHG140FVEB / RZQG125L8Y1B","FCQHG71FVEB / FCQHG71FVEB / RZQG125L8Y1B","FCQHG140FVEB / RZQG140L7Y1B"]
["Капацитет на охлаждане","Ном.","","кВт","","6.80","","","","","13.4"]
["Охлаждане с конвекция","SEER","","","7.00","6.91","7.00","5.10","6.61","5.10"]
["","Годишно потребление на електроенергия","","kWh/a","340","345","475","652","636","824"]
["","Капацитет","Pdesign","кВт","6.80","6.80","9.50","9.50","12.00","12.00"]
["","Клас на енергийна ефективност","","","A++","A++","A++","B","A++","B"]
["Отопление с конвекция (умерен климат)","Капацитет","Pdesign","кВт","7.60","7.60","11.30","11.30","12.66","12.71"]
["","SCOP/A","","","4.54","4.54","4.80","3.80","4.63","3.80"]
["","Клас на енергийна ефективност","","","A+","A+","A++","A","A++","A"]
["","Годишно потребление на електроенергия","","kWh/a","2,344","2,344","3,296","4,164","3,829","4,683"]
["Номинална ефективност","Годишен разход на енергия","","kWh","","830"]
["","EER","","","","4.09","","","","","3.35"]
["","COP","","","","4.80","","","","","4.12"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","","A"]
["","","Отопление","","","A"]
["Капацитет на отопление","Ном.","","кВт","","7.5","","","","","15.5"]
["Забележки","","","","","(1) - Годишният разход на електроенергия е съгласно Директивата за енергиен клас 2002/31/EC","","","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС"]
["","","","","","(2) - SEER и SCOP са съгласно EN 14825","","","","","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване"]