{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Капацитет на охлаждане","Общ капацитет","","Ном.","kW","12.10","19.00","22.00"]
["Топлинен капацитет","Общ капацитет","","Ном.","kW","13.50","22.4","24.0"]
["Корпус","Colour","","","","Небоядисан","Небоядисан","Небоядисан"]
["","Материал","","","","Галванизирана стомана","Галванизирана стоманена пластина","Галванизирана стоманена пластина"]
["Размери","Тяло","","Височина","мм","300","470","470"]
["","","","Широчина","мм","1,400","1,490","1,490"]
["","","","Дълбочина","мм","700","1,100","1,100"]
["Тегло","Тяло","","","кг","45","104","115"]
["Необходим окачен таван >","мм","","","","350"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","39.0","64.0","69.0"]
["","","","Среден","м³/мин","","50","56"]
["","","","Ниско","м³/мин","28.0","36.0","43.0"]
["","","Отопление","Висок","м³/мин","39.0","64.0","69.0"]
["","","","Среден","м³/мин","","50.0","56.0"]
["","","","Ниско","м³/мин","28.0","36.0","43.0"]
["","Външно статично налягане","","Високо","Pa","200","250","250"]
["","","","Ном.","Pa","50","62","62"]
["Звукова мощност","Охлаждане","","","дБА","66","69.0","71.0"]
["Ниво на звуково налягане","Охлаждане","","Висок","дБА","40","43.0","44.0"]
["","","","Среден","дБА","","39.0","40.0"]
["","","","Ниско","дБА","33","36.0","37.0"]
["","Отопление","","Висок","дБА","40","43.0","44.0"]
["","","","Среден","дБА","","39.0","40.0"]
["","","","Ниско","дБА","33","36.0","37.0"]
["Piping connections","Tечност","","Вън. д.","мм","9.52","9.52","9.52"]
["","Газ","","Вън. д.","мм","15.90","19.1","22.2"]
["","Дренаж","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Височина за източване","мм","","","","625"]
["Декоративен панел","Модел","","","","BYBS125DJW1"]
["","Цвят","","","","Бяло (10Y9/0,5)"]
["","Размери","","Височина","мм","55"]
["","","","Широчина","мм","1,500"]
["","","","Дълбочина","мм","500"]
["","Тегло","","","кг","6.5"]
["Системи за управление","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Стандартни аксесоари","Винтове","","","","16","2","2"]
["","Шайба","","","","8","12","12"]
["","Лента за маркуч","","","","1"]
["","Маркуч за източване","","","","1"]
["","Общи мерки за безопасност","","","","1","1","1"]
["","Ръководство за монтаж и работа","","","","1","1","1"]
["","Кабел за общо електрозахранване","","","","2"]
["","Материал за уплътнение (маркуч за източване)","","","","1"]
["","Материал за уплътнение","","","","2"]
["","Термоизолационна тръба (течност)","","","","1"]
["","Термоизолационна тръба (газ)","","","","1"]
["Power supply","Име","","","","","VE","VE"]
["","Фаза","","","","1~","1~","1~"]
["","Честота","","","Хц","50/60","50/60","50/60"]
["","Напрежение","","","V","220-240/220","220-240/220","220-240/220"]
["Забележки","","","","","(1) - Вж. отделния чертеж за електрическите схеми"]
["Стандартни аксесоари","Ръководство за работа","","","","","1","1"]
["","Ръководство за монтаж","","","","","1","1"]
["","Свързваща тръба за газ","","","","","1","1"]
["","Материал на телените скоби","","","","","1","1"]
["","Зегерка","","","","","2","2"]
["","Винт+Шайба","","","","","45","45"]
["","Винт с шестоъгълна глава с шайба","","","","","49","49"]
["","Винт с шестоъгълна глава","","","","","2","2"]
["","Обикновена шайба","","","","","8","8"]