{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RR-BW1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9/RR125B8W1B"]
["Капацитет на охлаждане","Ном.","","кВт","12.5 (1)"]
["Тръбни съединения","Tечност","Вън. д.","mm","9.52"]
["","Газ","Вън. д.","mm","15.9"]
["","Дренаж","вън. д.","mm","26"]
["Номинална ефективност","EER","","","2.61"]
["","Годишен разход на енергия","","kWh","2,395"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","D"]
["Забележки","","","","(1) - Охлаждане: температура на открито 27°C (сух термометър), 19°C (влажен термометър); външна температура 35°C със сух термометър; дължина на еквивал. тръбопр.: 7,5 м; денивелация: 0 м."]
["","","","","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване"]