{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":9,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F"]
[]
[]
[]
[]
["","","","","","FDXM25F2V1B","FDXM35F2V1B","FDXM50F2V1B","FDXM60F2V1B"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Ном.","м³/мин","8.0","8.0","11.0","14.8"]
["Ниво на звуково налягане","Охлаждане","","Ном.","dBA","33","33","36","35"]
["Вентилатор","Скорост на въздушния поток","Отопление","Ном.","м³/мин","8.0","8.0","14.8","14.8"]
["Ниво на звуково налягане","Отопление","","Ном.","dBA","33","33","36","36"]
["Входяща мощност","Охлаждане","","Ном.","кВт","0.036","0.036","0.060","0.060"]
["","Отопление","","Ном.","кВт","0.036","0.036","0.060","0.060"]
["Размери","Тяло","","Височина","мм","200","200","200","200"]
["","","","Широчина","мм","750","750","1150","1150"]
["","","","Дълбочина","мм","620","620","620","620"]
["Тегло","Тяло","","","кг","21","21","30","30"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","8.7","8.7","12.0","16.0"]
["","","","Ниско","м³/мин","7.3","7.3","10.0","13.5"]
["","","Отопление","Висок","м³/мин","8.7","8.7","16.0","16.0"]
["","","","Ниско","м³/мин","7.3","7.3","13.5","13.5"]
["","Външно статично налягане","","Ном.","Pa","30","30","40","40"]
["Звукова мощност","Охлаждане","","","dBA","53","53","55","56"]
["","Отопление","","","dBA","53","53","55","56"]
["Ниво на звуково налягане","Охлаждане","","Висок","dBA","35","35","38","38"]
["","","","Ниско","dBA","27","27","30","30"]
["","Отопление","","Висок","dBA","35","35","38","38"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","dBA","27","27","30","30"]
["Тръбни съединения","Tечност","","Вън. д.","мм","6.35","6.35","6.35","6.35"]
["","Газ","","Вън. д.","мм","9.5","9.5","12.7","12.7"]
["","Дренаж","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Системи за управление","Инфрачервено дистанционно управление","","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["","Жично дистанционно управление","","","","BRC1D52, BRC1E51A","BRC1D52, BRC1E51A","BRC1D52, BRC1E51A","BRC1D52, BRC1E51A"]
["Електрозахранване","Име","","","","V1","V1","V1","V1"]
["","Фаза","","","","1~","1~","1~","1~"]
["","Честота","","","Хц","50","50","50","50"]
["","Напрежение","","","V","230","230","220-240","220-240"]