{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B","FDXM35F3V1B","FDXM50F3V1B","FDXM60F3V1B"]
["Ниво на звуково налягане","Отопление","Висок","дБА","35","35","38","38"]
["","","Среден","дБА","33","33","35","35"]
["","","Ниско","дБА","27","27","30","30"]
["","Охлаждане","Среден","дБА","33","33","35","35"]
["","","Ниско","дБА","27","27","30","30"]
["","","Висок","дБА","35","35","38","38"]
["Стандартни аксесоари","Ръководство за монтаж","","","1","1","1","1"]
["","Ръководство за работа","","","1","1","1","1"]
["","Изолация за фитинг","","","1","1","1","1"]
["","Уплътняващ тампон","","","1","1","1","1"]
["","Метал за скоба","","","1","1","1","1"]
["","Маркуч за източване","","","1","1","1","1"]
["","Шайба за скоба за окачване","","","8","8","8","8"]
["","Материал за уплътнение","","","2","2","2","2"]
["","Скоби","","","6","6","6","6"]
["","Шайба за фиксиране на пластина","","","4","4","4","4"]
["","Винтове за тръбни фланци","","","1","1","1","1"]
["","Въздушен филтър","","","1","1","1","1"]
["Тръбни съединения","Tечност","Вън. д.","mm","6.35","6.35","6.35","6.35"]
["","Газ","Вън. д.","mm","9.50","9.50","12.70","12.70"]
["","Дренаж","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Входяща мощност","Охлаждане","Ном.","kW","0.036","0.036","0.060","0.060"]
["","Отопление","Ном.","kW","0.036","0.036","0.060","0.060"]
["Звукова мощност","Охлаждане","","дБА","53","53","55","56"]
["","Отопление","","дБА","53","53","55","56"]
["Размери","Тяло","Широчина","mm","750","750","1,150","1,150"]
["","","Дълбочина","mm","620","620","620","620"]
["","","Височина","mm","200","200","200","200"]
["Тегло","Тяло","","кг","21","21","28","28"]
["Вентилатор","Външно статично налягане","Ном.","Pa","30","30","40","40"]
["Power supply","Фаза","","","1~","1~","1~","1~"]
["","Честота","","Хц","50","50","50","50"]
["","Напрежение","","V","220-240","220-240","220-240","220-240"]