{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Ниво на звуково налягане","Отопление","","Висок","dBA","35.0","35.0","","38.0"]
["","","","Среден","dBA","33.0","33.0","","35.0"]
["","","","Ниско","dBA","27.0","27.0","","30.0"]
["","Охлаждане","","Среден","dBA","33.0","33.0","","35.0"]
["","","","Ниско","dBA","27.0","27.0","","30.0"]
["","","","Висок","dBA","35.0","35.0","","38.0"]
["Стандартни аксесоари","Ръководство за монтаж","","","","1","1","","1"]
["","Ръководство за работа","","","","1","1","","1"]
["","Изолация за фитинг","","","","1","1","","1"]
["","Уплътняващ тампон","","","","1","1","","1"]
["","Метал за скоба","","","","1","1","","1"]
["","Маркуч за източване","","","","1","1","","1"]
["","Шайба за скоба за окачване","","","","8","8","","8"]
["","Материал за уплътнение","","","","2","2","","2"]
["","Скоби","","","","6","6","","6"]
["","Шайба за фиксиране на пластина","","","","4","4","","4"]
["","Винтове за тръбни фланци","","","","1","1","","1"]
["","Въздушен филтър","","","","1","1","","1"]
["Тръбни съединения","Tечност","","Вън. д.","мм","6.35","6.35","","6.35"]
["","Газ","","Вън. д.","мм","9.50","9.50","","12.70"]
["","Дренаж","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Консумирана мощност","Охлаждане","","Ном.","кВт","0.036","0.036","","0.060"]
["","Отопление","","Ном.","кВт","0.036","0.036","","0.060"]
["Sound power level","Охлаждане","","","dBA","53.0","53.0","","56.0"]
["","Отопление","","","dBA","53.0","53.0","","56.0"]
["Размери","Тяло","","Широчина","мм","750","750","","1,150"]
["","","","Дълбочина","мм","620","620","","620"]
["","","","Височина","мм","200","200","","200"]
["Тегло","Тяло","","","кг","21","21","","28"]
["Вентилатор","Външно статично налягане","","Ном.","Pa","30","30","","40"]
["","Скорост на въздушния поток","Отопление","Висок","м³/мин","8.7","8.7","","16.0"]
["","","","Среден","м³/мин","8.0","8.0","","14.8"]
["","","","Ниско","м³/мин","7.3","7.3","","13.5"]
["","","Охлаждане","Ниско","м³/мин","7.3","7.3","","13.5"]
["","","","Среден","м³/мин","8.0","8.0","","14.8"]
["","","","Висок","м³/мин","8.7","8.7","","16.0"]
["Power supply","Фаза","","","","1~","1~","","1~"]
["","Честота","","","Хц","50","50","","50"]
["","Напрежение","","","V","220-240","220-240","","220-240"]
["Забележки","","","","","(1) - Вж. отделния чертеж за електрическите схеми","(1) - Вж. отделния чертеж за електрическите схеми","","(1) - Вж. отделния чертеж за електрическите схеми"]
["Входяща мощност","Охлаждане","","Ном.","кВт","","","0.060"]
["","Отопление","","Ном.","кВт","","","0.060"]
["Размери","Тяло","","Височина","мм","","","200"]
["","","","Широчина","мм","","","1150"]
["","","","Дълбочина","мм","","","620"]
["Тегло","Тяло","","","кг","","","28"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","","","15.8"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","","","14.6"]
["","","","Ниско","м³/мин","","","13.3"]
["","","Отопление","Висок","м³/мин","","","15.8"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","","","14.6"]
["","","Отопление","Ниско","м³/мин","","","13.3"]
["","Външно статично налягане","","Ном.","Pa","","","40"]
["Звукова мощност","Охлаждане","","","dBA","","","55.0"]
["","Отопление","","","dBA","","","55.0"]
["Ниво на звуково налягане","Охлаждане","","Висок","dBA","","","38.0"]
["","","","Среден","dBA","","","35.0"]
["","","","Ниско","dBA","","","30.0"]
["","Отопление","","Висок","dBA","","","38.0"]
["","","","Среден","dBA","","","35.0"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","dBA","","","30.0"]
["Тръбни съединения","Tечност","","Вън. д.","мм","","","6.35"]
["","Газ","","Вън. д.","мм","","","12.70"]
["","Дренаж","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Стандартни аксесоари","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Въздушен филтър","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["Електрозахранване","Фаза","","","","","","1~"]
["","Честота","","","Хц","","","50"]
["","Напрежение","","","V","","","220-240"]