{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RXS-L1"]
[]
[]
[]
[]
["","","","FDXS25F2VEB / RXS25L3V1B1","FDXS35F2VEB / RXS35L3V1B1"]
["Капацитет на охлаждане","Ном.","kW","2.60 (1)","3.20 (1)"]
["Номинална ефективност","EER","","4.10","3.41"]
["","COP","","4.00","3.31"]
["Топлинен капацитет","Ном.","kW","3.15 (2)","3.75 (2)"]
["Забележки","","","(1) - Вътрешна температура: 27°CDB, 19°CWB; външна температура: 35°CDB, 24°CWB","(1) - Вътрешна температура: 27°CDB, 19°CWB; външна температура: 35°CDB, 24°CWB"]
["","","","(2) - Вътрешна температура: 20°CDB, 15°CWB; външна температура: 7°CDB, 6°CWB.","(2) - Вътрешна температура: 20°CDB, 15°CWB; външна температура: 7°CDB, 6°CWB."]