{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":10,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG71L8Y1B","FDXS35F2VEB / FDXS35F2VEB / RZQG71L8Y1B","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG100L8Y1B","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG100L8Y1B","FDXS60F2VEB / FDXS60F2VEB / RZQG125L8Y1B","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG125L8Y1B (Archived)"]
["Охлаждане с конвекция","SEER","","","4.80","4.8","5.10"]
["","Годишно потребление на електроенергия","","kWh/a","496","496","652"]
["","Капацитет","Pdesign","кВт","6.80","6.8","9.50"]
["","Клас на енергийна ефективност","","","B","B","B"]
["Отопление с конвекция (умерен климат)","Капацитет","Pdesign","кВт","6.00","6","10.74"]
["","SCOP/A","","","3.80","3.8","3.80"]
["","Клас на енергийна ефективност","","","A","A","A"]
["","Годишно потребление на електроенергия","","kWh/a","2,211","2,211","3,957"]
["Забележки","","","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС"]
["Охлаждане с конвекция","Клас на енергийна ефективност","","","","","","B","B","B"]
["","Капацитет","Pdesign","кВт","","","","9.5","12","12.00"]
["","SEER","","","","","","5.1","5.1","5.10"]
["","Годишно потребление на електроенергия","","kWh/a","","","","652","824","824"]
["Отопление с конвекция (умерен климат)","Клас на енергийна ефективност","","","","","","A","A","A"]
["","Капацитет","Pdesign","кВт","","","","10.74","12.71","11.30"]
["","SCOP/A","","","","","","3.8","3.8","3.80"]
["","Годишно потребление на електроенергия","","kWh/a","","","","3957","4683","4164"]
["Диапазон на енергийна ефективност","","","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Външно тяло","","","","","","","","","RZQG125L8Y1"]