{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9 / RXS-L"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9 / RXS50L2V1B"]
["Капацитет на охлаждане","Мин.","","kW","1.7"]
["","Макс.","","kW","5.3"]
["","Ном.","","kW","5.0"]
["Тръбни връзки","Tечност","Вън. д.","мм","6.35"]
["","Газ","Вън. д.","мм","12.7"]
["","Дренаж","вън. д.","мм","VP20 (Външен диам. 26, Вътр. диам. 20)"]
["Номинална ефективност","Годишен разход на енергия","","kWh","825"]
["","EER","","","3.03"]
["","COP","","","3.10"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","B"]
["","","Отопление","","D"]
["Топлинен капацитет","Ном.","","kW","5.8"]
["","Мин.","","kW","1.7"]
["","Макс.","","kW","6.0"]
["Забележки","","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС"]
["","","","","(2) - 230V"]
["","","","","(3) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване"]