{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":14,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG100L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG125L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / FFA50A2VEB9 / RZQG125L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / RZQG100L8Y1B","FFA60A2VEB9 / FFA60A2VEB9 / RZQG125L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG100L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / FFA50A2VEB9 / RZQG100L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG71L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / RZQG71L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / RZQG71L8Y1B"]
["Диапазон на енергийна ефективност","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Капацитет на охлаждане","Ном.","","кВт","","","","","","","","6.80","6.80","6.80"]
["Охлаждане с конвекция","SEER","","","","","","","","","","5.10","5.10","5.10"]
["","Годишно потребление на електроенергия","","kWh/a","","","","","","","","467","467","467"]
["","Капацитет","Pdesign","кВт","","","","","","","","6.80","6.80","6.80"]
["","Клас на енергийна ефективност","","","","","","","","","","A","A","A"]
["Отопление с конвекция (умерен климат)","Капацитет","Pdesign","кВт","","","","","","","","6.00","6.00","6.00"]
["","SCOP/A","","","","","","","","","","3.80","3.80","3.80"]
["","Клас на енергийна ефективност","","","","","","","","","","A","A","A"]
["","Годишно потребление на електроенергия","","kWh/a","","","","","","","","2,211","2,211","2,211"]
["Номинална ефективност","EER","","","","","","","","","","3.38","3.38","3.38"]
["Забележки","","","","","","","","","","","(1) - Вж. отделния чертеж за работен диапазон","(1) - Номиналният капацитет на охлаждане се базира на: вътрешна температура: 27°CDB, 19°CWB, външна температура: 35°CDB, еквивалентна дължина на тръбите за хладилен агент: 5 m, разлика в нивото: 0m.","(1) - Вж. отделния чертеж за работен диапазон"]
["","","","","","","","","","","","(2) - Вж. отделния чертеж за електрическите схеми","(2) - Номиналният капацитет за загряване важи за: вътрешна температура: 20°C (сух термометър), външна температура: 7°C (сух термометър), 8°C (влажен термометър), съответна дължина на тръбите: 5 м, денивелация: 0m.","(2) - Вж. отделния чертеж за електрическите схеми"]
["","","","","","","","","","","","","(3) - Вж. отделния чертеж за работен диапазон"]
["","","","","","","","","","","","","(4) - Вж. отделния чертеж за електрическите схеми"]