{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":17,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG125L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG100L8Y1B","FHA50AVEB / FHA50AVEB / RZQG100L8Y1B","FHA50AVEB / FHA50AVEB / FHA50AVEB / RZQG125L8Y1B","FHA60AVEB / FHA60AVEB / RZQG125L8Y1B","FHA35AVEB / FHA35AVEB / RZQG71L8Y1B","FHA50AVEB / FHA50AVEB / RZQG71L8Y1B","FHA71AVEB / RZQG71L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG71L8Y1B","FHA71AVEB / FHA71AVEB / RZQG100L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG100L8Y1B","FHA50AVEB / FHA50AVEB / FHA50AVEB / RZQG100L8Y1B","FHA71AVEB / FHA71AVEB / RZQG125L8Y1B"]
["Диапазон на енергийна ефективност","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","","","","","","A+++ ~ D"]
["Охлаждане с конвекция","SEER","","","","","","","","5.10","5.10","6.86","5.10","5.10","5.10","5.10"]
["","Годишно потребление на електроенергия","","kWh/a","","","","","","467","467","347","467","652","652","652"]
["","Капацитет","Pdesign","кВт","","","","","","6.80","6.80","6.80","6.80","9.50","9.50","9.50"]
["","Клас на енергийна ефективност","","","","","","","","A","A","A++","A","A","A","A"]
["Отопление с конвекция (умерен климат)","Капацитет","Pdesign","кВт","","","","","","6.00","6.00","7.60","6.00","11.30","11.30","11.30"]
["","SCOP/A","","","","","","","","3.80","3.80","4.32","3.80","3.80","3.80","3.80"]
["","Клас на енергийна ефективност","","","","","","","","A","A","A+","A","A","A","A"]
["","Годишно потребление на електроенергия","","kWh/a","","","","","","2,211","2,211","2,463","2,211","4,164","4,164","4,164"]
["Забележки","","","","","","","","","(1) - Охлаждане: температура на открито 27°C (сух термометър), 19°C (влажен термометър); външна температура 35°C със сух термометър; дължина на еквивал. тръбопр.: 7,5 м; денивелация: 0 м.","","(1) - Охлаждане: температура на открито 27°C (сух термометър), 19°C (влажен термометър); външна температура 35°C със сух термометър; дължина на еквивал. тръбопр.: 7,5 м; денивелация: 0 м."]
["","","","","","","","","","(2) - Отопление: температура на открито 20°С (сух термометър), външна темп. 7°C (сух термометър), 6°C (влажен термометър); съответна дължина на тръбите за хладилния агент: 7,5 м; денивелация: 0 м.","","(2) - Отопление: температура на открито 20°С (сух термометър), външна темп. 7°C (сух термометър), 6°C (влажен термометър); съответна дължина на тръбите за хладилния агент: 7,5 м; денивелация: 0 м."]
["","","","","","","","","","(3) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","","(3) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС"]
["Капацитет на охлаждане","Ном.","","кВт","","","","","","","","6.80 (1)"]
["Номинална ефективност","Годишен разход на енергия","","kWh","","","","","","","","890"]
["","EER","","","","","","","","","","3.82 (3)"]
["","COP","","","","","","","","","","4.13 (3)"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","","","","","","","","A"]
["","","Отопление","","","","","","","","","A"]
["Капацитет на отопление","Ном.","","кВт","","","","","","","","7.50 (2)"]
["Охлаждане с конвекция","Клас на енергийна ефективност","","","","","","","","","","","","","","","A"]
["","Капацитет","Pdesign","кВт","","","","","","","","","","","","","12.00"]
["","SEER","","","","","","","","","","","","","","","5.10"]
["","Годишно потребление на електроенергия","","kWh/a","","","","","","","","","","","","","824"]
["Отопление с конвекция (умерен климат)","Клас на енергийна ефективност","","","","","","","","","","","","","","","A"]
["","Капацитет","Pdesign","кВт","","","","","","","","","","","","","12.71"]
["","SCOP/A","","","","","","","","","","","","","","","3.80"]
["","Pdh Капацитет на отопление при -10°","","кВт","","","","","","","","","","","","","11"]
["","Годишно потребление на електроенергия","","kWh/a","","","","","","","","","","","","","4683"]