{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A"]
[]
[]
[]
[]
["","","","","FHA35AVEB","FHA50AVEB","FHA60AVEB","FHA71AVEB"]
["Ниво на звуково налягане","Отопление","Висок","dBA","36","37","37","38"]
["","","Ном.","dBA","34","35","35","36"]
["","","Среден","dBA","31","32","33","34"]
["","Охлаждане","Среден","dBA","34","35","35","36"]
["","","Ниско","dBA","31","32","33","34"]
["","","Висок","dBA","36","37","37","38"]
["Стандартни аксесоари","Термоизолационна тръба","","","2","2","2","2"]
["","Материал на телените скоби","","","7","7","7","7"]
["","Лента за маркуч","","","1","1","1","1"]
["","Маркуч за източване","","","1","1","1","1"]
["","Шайба","","","8","8","8","8"]
["","Уплътняващ тампон (голям)","","","1","1","1","1"]
["","Уплътняващ тампон (малък)","","","1","1","1","1"]
["","Гумена втулка","","","1","1","1","1"]
["","Винтове","","","2","2","2","2"]
["","Арматурно фиксиращо приспособление","","","2","2","2","2"]
["Control systems","Wired remote control","","","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7"]
["","Infrared remote control","","","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56"]
["Тръбни съединения","Tечност","Вън. д.","мм","6.35","6.35","6.35","9.52"]
["","Газ","Вън. д.","мм","9.50","12.7","12.7","15.9"]
["","Дренаж","","","VP20","VP20","VP20","VP20"]
["Звукова мощност","Охлаждане","","dBA","53","54","54","55"]
["Размери","Тяло","Широчина","мм","960","960","1,270","1,270"]
["","","Дълбочина","мм","690","690","690","690"]
["","","Височина","мм","235","235","235","235"]
["Корпус","Материал","","","Смола, ламарина","Смола, ламарина","Смола, ламарина","Смола, ламарина"]
["","Colour","","","Бяло","Бяло","Бяло","Бяло"]
["Тегло","Тяло","","кг","24.0","25.0","31.0","32.0"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Честота","","Хц","50","50","50","50"]
["","Напрежение","","V","220-240","220-240","220-240","220-240"]
["Забележки","","","","(1) - Вж. отделния чертеж за електрическите схеми","(1) - Вж. отделния чертеж за електрическите схеми","(1) - Вж. отделния чертеж за електрическите схеми","(1) - Вж. отделния чертеж за електрическите схеми"]