{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RXS-F"]
[]
[]
[]
[]
["","","","","FHQ60CAVEB / RXS60F4V1B"]
["Капацитет на охлаждане","Ном.","","kW","5.7"]
["Топлинен капацитет","Ном.","","kW","7.2"]
["Номинална ефективност","EER","","","3.26"]
["","COP","","","3.32"]
["","Годишен разход на енергия","","kWh","875"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","A"]
["","","Отопление","","C"]
["Охлаждане с конвекция","Клас на енергийна ефективност","","","A"]
["","Капацитет","Pdesign","kW","7.20"]
["","SEER","","","5.54"]
["","Годишно потребление на електроенергия","","kWh/a","360"]
["Отопление с конвекция (умерен климат)","Клас на енергийна ефективност","","","A"]
["","Капацитет","Pdesign","kW","5.07"]
["","SCOP/A","","","3.50"]
["","Годишно потребление на електроенергия","","kWh/a","2026.36"]
["Забележки","","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС"]
["","","","","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване"]