{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":14,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RZQG-L8/7V1"]
[]
[]
[]
[]
["","","","","FHQ35CAVEB / FHQ35CAVEB / RZQG71L8V1B","FHQ71CAVEB / RZQG71L8V1B","FHQ100CAVEB / RZQG100L8V1B","FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / RZQG100L8V1B","FHQ50CAVEB / FHQ50CAVEB / RZQG100L8V1B","FHQ125CAVEB / RZQG125L8V1B","FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / RZQG125L8V1B","FHQ50CAVEB / FHQ50CAVEB / FHQ50CAVEB / RZQG125L8V1B","FHQ60CAVEB / FHQ60CAVEB / RZQG125L8V1B","FHQ140CAVEB / RZQG140L7V1B"]
["Капацитет на охлаждане","Ном.","","kW","","6.8","9.5","","","12.0","","","","13.4"]
["Охлаждане с конвекция","SEER","","","5.10","6.95","6.11","5.10","5.10","6.01","5.10","5.10","5.10"]
["","Годишно потребление на електроенергия","","kWh/a","467","342.446","544.19","652","652","698.835","824","824","824"]
["","Капацитет","Pdesign","kW","6.80","6.80","9.50","9.50","9.50","12.00","12.00","12.00","12.00"]
["","Клас на енергийна ефективност","","","A","A++","A++","A","A","A+","A","A","A"]
["Отопление с конвекция (умерен климат)","Капацитет","Pdesign","kW","6.00","7.60","11.30","11.30","11.30","14.13","12.71","12.71","12.71"]
["","SCOP/A","","","3.80","4.32","4.61","3.80","3.80","4.23","3.80","3.80","3.80"]
["","Клас на енергийна ефективност","","","A","A+","A++","A","A","A+","A","A","A"]
["","Годишно потребление на електроенергия","","kWh/a","2,211","2,462.963","3,431.67","4,163","4,163","4,676.596","4,683","4,683","4,683"]
["Номинална ефективност","Годишен разход на енергия","","kWh","","890","1,245","","","1,790","","","","2,025"]
["","EER","","","","3.82","3.81","","","3.35","","","","3.31"]
["","COP","","","","4.13","4.15","","","3.89","","","","3.63"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","","A","A","","","A"]
["","","Отопление","","","A","A","","","A"]
["Топлинен капацитет","Ном.","","kW","","7.5","10.8","","","13.5","","","","15.5"]
["Забележки","","","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС"]
["","","","","","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване","","","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване","","","","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване"]
["","","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС"]