{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":12,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RZQSG-L(3/8)V1"]
[]
[]
[]
[]
["","","","","FHQ35CAVEB / FHQ35CAVEB / RZQSG71L3V1B","FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / RZQSG100L8V1B","FHQ50CAVEB / FHQ50CAVEB / RZQSG100L8V1B","FHQ125CAVEB / RZQSG125L8V1B","FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / RZQSG125L8V1B","FHQ50CAVEB / FHQ50CAVEB / FHQ50CAVEB / RZQSG125L8V1B","FHQ60CAVEB / FHQ60CAVEB / RZQSG125L8V1B","FHQ140CAVEB / RZQSG140L7V1B"]
["Капацитет на охлаждане","Ном.","","кВт","","","","12.0","","","","13.4"]
["Охлаждане с конвекция","SEER","","","5.10","5.10","5.10","5.61","4.80","4.80","4.80"]
["","Годишно потребление на електроенергия","","kWh/a","467","652","652","748.663","875","875","875"]
["","Капацитет","Pdesign","кВт","6.80","9.50","9.50","12.00","12.00","12.00","12.00"]
["","Клас на енергийна ефективност","","","A","A","A","A+","B","B","B"]
["Отопление с конвекция (умерен климат)","Капацитет","Pdesign","кВт","6.00","7.60","7.60","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","3.80","3.80","3.80","4.01","3.80","3.80","3.80"]
["","Клас на енергийна ефективност","","","A","A","A","A+","A","A","A"]
["","Годишно потребление на електроенергия","","kWh/a","2,211","2,800","2,800","2,653.367","2,800","2,800","2,800"]
["Номинална ефективност","Годишен разход на енергия","","kWh","","","","2,075"]
["","EER","","","","","","2.89","","","","3.01"]
["","COP","","","","","","3.62","","","","3.41"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","","","","C"]
["","","Отопление","","","","","A"]
["Топлинен капацитет","Ном.","","кВт","","","","13.5","","","","15.5"]
["Забележки","","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС"]
["","","","","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване","","","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване","","","","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване"]
["","","","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС"]