{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":12,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-CB / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHQ100CBVEB / RZQSG100L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQSG100L8Y1B","FHQ50CBVEB / FHQ50CBVEB / RZQSG100L8Y1B","FHQ125CBVEB / RZQSG125L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQSG125L8Y1B","FHQ50CBVEB / FHQ50CBVEB / FHQ50CBVEB / RZQSG125L8Y1B","FHQ60CBVEB / FHQ60CBVEB / RZQSG125L8Y1B","FHQ140CBVEB / RZQSG140L7Y1B"]
["Капацитет на охлаждане","Ном.","","кВт","9.5","","","12.0","","","","13.4"]
["Охлаждане с конвекция","SEER","","","5.61","5.10","5.10","5.61","4.80","4.80","4.80"]
["","Годишно потребление на електроенергия","","kWh/a","593","652","652","749","875","875","875"]
["","Капацитет","Pdesign","кВт","9.5","9.50","9.50","12","12.00","12.00","12.00"]
["","Клас на енергийна ефективност","","","A+","B","B","A+","B","B","B"]
["Отопление с конвекция (умерен климат)","Капацитет","Pdesign","кВт","7.6","7.60","7.60","7.6","7.60","7.60","7.60"]
["","SCOP/A","","","3.91","3.80","3.80","4.01","3.80","3.80","3.80"]
["","Клас на енергийна ефективност","","","A","A","A","A+","A","A","A"]
["","Годишно потребление на електроенергия","","kWh/a","2,722","2,800","2,800","2,654","2,800","2,800","2,800"]
["Номинална ефективност","Годишен разход на енергия","","kWh","1,480","","","2,075","","","","2,225"]
["","EER","","","3.21","","","2.89","","","","3.01"]
["","COP","","","3.61","","","3.62","","","","3.41"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","A","","","C","","","","B"]
["","","Отопление","","A","","","A","","","","B"]
["Капацитет на отопление","Ном.","","кВт","10.8","","","13.5","","","","15.5"]
["Забележки","","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС"]
["","","","","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване","","","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване","","","","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване"]