{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9 / RXS-L"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9 / RXS35L2V1B"]
["Капацитет на охлаждане","Мин.","","кВт","1.2"]
["","Макс.","","кВт","3.8"]
["","Ном.","","кВт","3.5"]
["Тръбни съединения","Tечност","Вън. д.","мм","6.35"]
["","Газ","Вън. д.","мм","9.5"]
["","Дренаж","вън. д.","мм","18.0"]
["Номинална ефективност","Годишен разход на енергия","","kWh","565"]
["","EER","","","3.10"]
["","COP","","","3.57"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","B"]
["","","Отопление","","B"]
["Топлинен капацитет","Ном.","","кВт","4.0"]
["","Мин.","","кВт","1.4"]
["","Макс.","","кВт","5.0"]
["Забележки","","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС"]
["","","","","(2) - 220V"]
["","","","","(3) - 230V"]
["","","","","(4) - 240V"]
["","","","","(5) - Охлаждане: температура на открито 27°C със сух термометър, 19.0°C с влажен термометър; външна темп. 35°C със сух термометър; 24°C с влажен термометър; съответстваща дължина на тръбопр.: 5м"]
["","","","","(6) - Отопление: температура на открито 20°С (сух термометър), външна темп. 7°C (сух термометър), 6°C (влажен термометър); съответна дължина на тръбите за хладилния агент: 5м"]
["","","","","(7) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване"]