{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9 / RXM-A"]
[]
[]
[]
[]
["","","","","FNA50A2VEB9 / RXM50A5V1B","FNA60A2VEB9 / RXM60A5V1B"]
["Капацитет на охлаждане","Ном.","","кВт","5.00","6"]
["Топлинен капацитет","Ном.","","кВт","5.80","7"]
["Номинална ефективност","EER","","","3.38","2.7"]
["","COP","","","3.34","3.11"]
["","Годишен разход на енергия","","kWh","740","1111"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","A","D"]
["","","Отопление","","C","D"]
["Охлаждане с конвекция","Клас на енергийна ефективност","","","A+","A"]
["","Капацитет","Pdesign","кВт","5.00","6"]
["","SEER","","","5.77","5.56"]
["","Годишно потребление на електроенергия","","kWh/a","303","378"]
["Отопление с конвекция (умерен климат)","Клас на енергийна ефективност","","","A+","A+"]
["","Капацитет","Pdesign","кВт","4.00","4.6"]
["","SCOP/A","","","4.09","4.16"]
["","Pdh Капацитет на отопление при -10°","","кВт","3.54","3.94"]
["","Годишно потребление на електроенергия","","kWh/a","1368","1547"]
["Забележки","","","","","(1) - Номиналният капацитет на охлаждане се базира на: вътрешна темп.: 27°CDB, 19°CWB, външна температура: 35°CDB, еквивалентна дължина на тръбите за хладилен агент: 5 m, разлика в нивото: 0m."]
["","","","","","(2) - Номиналният капацитет за загряване важи за: вътрешна температура: 20°C (сух термометър), външна температура: 7°C (сух термометър), 8°C (влажен термометър), съответна дължина на тръбите: 5 м, денивелация: 0m."]
["","","","","","(3) - Вж. отделния чертеж за работен диапазон"]
["","","","","","(4) - Вж. отделния чертеж за електрическите схеми"]