{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":9,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9"]
[]
[]
[]
[]
["","","","","","FNA25A2VEB9","FNA35A2VEB9","FNA50A2VEB9","FNA60A2VEB9"]
["Ниво на звуково налягане","Отопление","","Висок","дБА","33.0","33.0","36.0","36.0"]
["","","","Ном.","дБА","31.0","31.0","33.0","33.0"]
["","","","Ниско","дБА","28.0","28.0","30.0","30.0"]
["","Охлаждане","","Среден","дБА","31.0","31.0","33.0","33.0"]
["","","","Ниско","дБА","28.0","28.0","30.0","30.0"]
["","","","Висок","дБА","33.0","33.0","36.0","36.0"]
["Системи за управление","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["","Infrared remote control","","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Piping connections","Tечност","","Вън. д.","мм","6.35","6.35","6.35","6.35"]
["","Газ","","Вън. д.","мм","9.52","9.52","12.7","12.7"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Звукова мощност","Охлаждане","","","дБА","53.0","53.0","56.0","56.0"]
["Размери","Тяло","","Широчина","мм","790","790","1,190","1,190"]
["","","","Дълбочина","мм","200","200","200","200"]
["","","","Височина","мм","620, 720 (1)","620, 720 (1)","620, 720 (1)","620, 720 (1)"]
["Корпус","Материал","","","","Галванизирана стоманена пластина","Галванизирана стоманена пластина","Галванизирана стоманена пластина","Галванизирана стоманена пластина"]
["","Colour","","","","Небоядисан","Небоядисан","Небоядисан","Небоядисан"]
["Тегло","Тяло","","","кг","23.0","23.0","30.0","30.0"]
["Вентилатор","Външно статично налягане","","Високо","Pa","48","48","49","49"]
["","","","Ном.","Pa","30","30","40","40"]
["","Скорост на въздушния поток","Отопление","Висок","м³/мин","8.7","8.7","16.0","16.0"]
["","","","Ниско","м³/мин","7.3","7.3","13.5","13.5"]
["","","","Ном.","м³/мин","8.0","8.0","14.8","14.8"]
["","","Охлаждане","Ниско","м³/мин","7.3","7.3","13.5","13.5"]
["","","","Ном.","м³/мин","8.0","8.0","14.8","14.8"]
["","","","Висок","м³/мин","8.7","8.7","16.0","16.0"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Име","","","","VE","VE","VE","VE"]
["","Честота","","","Хц","50/60","50/60","50/60","50/60"]
["","Напрежение","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Забележки","","","","","(1) - Включително крака за монтаж","(1) - Включително крака за монтаж","(1) - Включително крака за монтаж","(1) - Включително крака за монтаж"]
["","","","","","(2) - Нивото на силата на звука е абсолютна стойност, която означава силата на звука, който източникът на звук генерира.","(2) - Нивото на силата на звука е абсолютна стойност, която означава силата на звука, който източникът на звук генерира.","(2) - Нивото на силата на звука е абсолютна стойност, която означава силата на звука, който източникът на звук генерира.","(2) - Нивото на силата на звука е абсолютна стойност, която означава силата на звука, който източникът на звук генерира."]