{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNQ-A"]
[]
[]
[]
[]
["","","","","FNQ25A2VEB","FNQ35A2VEB","FNQ50A2VEB","FNQ60A2VEB"]
["Ниво на звуково налягане","Отопление","Висок","дБА","33","33","36","36"]
["","","Ном.","дБА","31","31","33","33"]
["","","Ниско","дБА","28","28","30","30"]
["","Охлаждане","Ниско","дБА","28","28","30","30"]
["","","Висок","дБА","33","33","36","36"]
["","","Ном.","дБА","31","31","33","33"]
["Хладилен агент","Потенциал на глобално затопляне","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["Системи за управление","Wired remote control","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Капацитет на охлаждане","Общ капацитет","Ном.","kW","2.6","3.4","5.0","6.0"]
["Тръбни съединения","Tечност","Вън. д.","mm","6.35","6.35","6.35","6.35"]
["","Газ","Вън. д.","mm","9.52","9.52","12.7","12.7"]
["","Дренаж","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Звукова мощност","Охлаждане","","дБА","53","53","56","56"]
["Размери","Тяло","Широчина","mm","790","790","1,190","1,190"]
["","","Дълбочина","mm","200","200","200","200"]
["","","Височина","mm","620, 720 (2)","620, 720 (2)","620, 720 (2)","620, 720 (2)"]
["Корпус","Материал","","","Галванизирана стоманена пластина","Галванизирана стоманена пластина","Галванизирана стоманена пластина","Галванизирана стоманена пластина"]
["","Цвят","","","Небоядисан","Небоядисан","Небоядисан","Небоядисан"]
["Тегло","Тяло","","кг","23","23","30","30"]
["Вентилатор","Външно статично налягане","Високо","Pa","48","48","49","49"]
["","","Ном.","Pa","30","30","40","40"]
["Топлинен капацитет","Общ капацитет","Ном.","kW","3.2","4.0","5.8","7.0"]
["Power supply","Фаза","","","1~","1~","1~","1~"]
["","Честота","","Хц","50/60","50/60","50/60","50/60"]
["","Напрежение","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Забележки","","","","(1) - Нивото на силата на звука е абсолютна стойност, която означава силата на звука, който източникът на звук генерира.","(1) - Нивото на силата на звука е абсолютна стойност, която означава силата на звука, който източникът на звук генерира.","(1) - Нивото на силата на звука е абсолютна стойност, която означава силата на звука, който източникът на звук генерира.","(1) - Нивото на силата на звука е абсолютна стойност, която означава силата на звука, който източникът на звук генерира."]
["","","","","(2) - Включително крака за монтаж","(2) - Включително крака за монтаж","(2) - Включително крака за монтаж","(2) - Включително крака за монтаж"]