{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":10,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-GV"]
[]
[]
[]
[]
["","","","","FTX50GV1B","FTX60GV1B","FTX71GV1B","FTX20GV1B (Archived)","FTX25GV1B (Archived)","FTX35GV1B (Archived)"]
["Ниво на звуково налягане","Отопление","Висок","дБА","42","44","46","39","40","41"]
["","","Тих режим","дБА","30","32","34","25","25","26"]
["","","Ниско","дБА","33","35","37","28","28","29"]
["","Охлаждане","Тих режим","дБА","31","33","34","22","22","23"]
["","","Ниско","дБА","34","36","37","25","26","27"]
["","","Висок","дБА","43","45","46","39","40","41"]
["","","Ном.","дБА","38","40","42","34","34","35"]
["","Охлаждане","Ном.","дБА","39","41","42","33","33","34"]
["Стандартни аксесоари","Ръководство за монтаж","","","1","1","1","1","1","1"]
["","Ръководство за работа","","","1","1","1","1","1","1"]
["","Безжично дистанционно управление","","","1","1","1","1","1","1"]
["","Батерии","","","2","2","2","2","2","2"]
["","Стойка за дистанционното","","","1","1","1","1","1","1"]
["","Монтажна пластина:","","","1","1","1","1","1","1"]
["","Фиксиращ винт за вътрешното устройство","","","","","","2","2","2"]
["","Филтър за фотокаталитично пречистване на въздуха от титанов апатит","","","2","2","2","2","2","2"]
["Системи за управление","Infrared remote control","","","ARC433B70","ARC433B70","ARC433B70"]
["Тръбни връзки","Tечност","Вън. д.","мм","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Газ","Вън. д.","мм","12.7","12.7","15.9","9.52","9.52","9.52"]
["","Дренаж","","","18","18","18","18","18","18"]
["Power input","Охлаждане","Ном.","kW","0.034","0.040 (2), 0.040 (3), 0.040 (4)","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Отопление","Ном.","kW","0.036","0.045 (2), 0.045 (3), 0.045 (4)","0.060 (2), 0.060 (3), 0.06 (4)"]
["Sound power level","Охлаждане","","дБА","59","60","63","55","56","57"]
["","Отопление","","дБА","58","59","62","55","56","57"]
["Размери","Тяло","Широчина","мм","1,050","1,050","1,050","770","770","770"]
["","","Дълбочина","мм","238","238","238","198","198","198"]
["","","Височина","мм","290","290","290","283","283","283"]
["Корпус","Цвят","","","Бяло","Бяло","Бяло","Бяло","Бяло","Бяло"]
["Тегло","Тяло","","kg","12","12","12","7","7","7"]
["Power supply","Фаза","","","1~","1~","1~","1~","1~","1~"]
["","Честота","","Хц","50","50","50","50","50","50"]
["","Име","","","V1","V1","V1","V1","V1","V1"]
["","Напрежение","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Стандартни аксесоари","Фиксиращи винтове за вътрешното устройство","","","2","2"]
["Забележки","","","","(1) - SL: Настройка за тихо ниво на темпото на въздушен поток","(1) - SL: Настройка за тихо ниво на темпото на въздушен поток","(1) - SL: Настройка за тихо ниво на темпото на въздушен поток"]
["","","","","(2) - 220V","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V","(4) - 240V"]
["Стандартни аксесоари","Фиксиращи винтове за вътрешното тяло (M4 x 12L)","","","","","2"]