{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":16,"n_cols":15,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-AW / RXA-A"]
[]
[]
[]
[]
["","","","","FTXA20A2V1BW / RXA20A2V1B","FTXA20A2V1BW / RXA20A3V1B","FTXA20A2V1BW / RXA20A5V1B","FTXA25A2V1BW / RXA25A3V1B","FTXA25A2V1BW / RXA25A5V1B","FTXA35A2V1BW / RXA35A2V1B","FTXA35A2V1BW / RXA35A3V1B","FTXA35A2V1BW / RXA35A5V1B","FTXA42A2V1BW / RXA42A2V1B","FTXA50A2V1BW / RXA50A2V1B","FTXA25A2V1BW / RXA25A2V1B (Archived)"]
["Капацитет на охлаждане","Мин.","","kW","1.3","1.3","1.3","1.3","1.3","1.4","1.4","1.4","1.7","1.7","1.3"]
["","Макс.","","kW","2.6","2.6","2.6","3.2","3.2","4.0","4.0","4.0","5.0","5.3","3.2"]
["","Ном.","","kW","2.0","2.0","2.0","2.5","2.5","3.4","3.4","3.4","4.2","5.0","2.5"]
["Номинална ефективност","EER","","","4.70","4.70","4.70","4.46","4.46","4.37","4.37","4.37","3.99","3.68","4.46"]
["","COP","","","5.00","5.00","5.00","5.00","5.00","4.04","4.04","4.04","4.12","4.00","5.00"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","A","A","A","A","A","A","A","A","A","A","A"]
["","","Отопление","","A","A","A","A","A","A","A","A","A","A","A"]
["Топлинен капацитет","Ном.","","kW","2.50","2.50","2.50","2.80","2.80","4.00","4.00","4.00","5.40","5.80","2.80"]
["","Мин.","","kW","1.30","1.30","1.30","1.30","1.30","1.40","1.40","1.40","1.70","1.70","1.30"]
["","Макс.","","kW","3.50","3.50","3.50","4.70","4.70","5.20","5.20","5.20","6.00","6.50","4.70"]