{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":92,"n_cols":10,"rows_kept":92,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-AW"]
[]
[]
[]
[]
["","","","","","FTXA20A2V1BW","FTXA25A2V1BW","FTXA35A2V1BW","FTXA42A2V1BW","FTXA50A2V1BW"]
["Ниво на звуково налягане","Отопление","","Висок","дБА","39","40","41","","46"]
["","","","Среден","дБА","32","33","33","","42"]
["","","","Тих режим","дБА","19","19","19","","24"]
["","","","Ниско","дБА","25","25","25","","33"]
["","Охлаждане","","Среден","дБА","32","33","33","","39"]
["","","","Тих режим","дБА","19","19","19","","24"]
["","","","Ниско","дБА","25","25","25","","31"]
["","","","Висок","дБА","39","40","41","","46"]
["Стандартни аксесоари","Ръководство за монтаж","","","","1","1","1","","1"]
["","Ръководство за работа","","","","1","1","1","","1"]
["","Въздушен филтър","","","","2","2","2","","2"]
["","Инфрачервено дистанционно","","","","1","1","1","","1"]
["","Монтажна пластина за дистанционно","","","","1","1","1","","1"]
["","Плик за винтове","","","","1","1","1","","1"]
["","Винтов капак","","","","1","1","1","","1"]
["","Сухи батерии тип ААА","","","","2","2","2","","2"]
["","Общи мерки за безопасност","","","","1","1","1","","1"]
["Хладилен агент","Потенциал на глобално затопляне","","","","675.0","675.0","675.0","","675.0"]
["Системи за управление","Wired remote control","","","","BRC073","BRC073","BRC073","","BRC073"]
["","Infrared remote control","","","","ARC466A58","ARC466A58","ARC466A58","","ARC466A58"]
["Piping connections","Tечност","","Вън. д.","мм","6.35","6.35","6.35","","6.35"]
["","Газ","","Вън. д.","мм","9.50","9.50","9.50","","12.70"]
["","Дренаж","","","","18","18","18","","18"]
["Входяща мощност","Охлаждане","","Ном.","kW","0.020","0.022","0.023","","0.030"]
["","Отопление","","Ном.","kW","0.020","0.020","0.022","","0.039"]
["Звукова мощност","Охлаждане","","","дБА","57","57","60","","60"]
["Размери","Тяло","","Широчина","мм","798","798","798","","798"]
["","","","Дълбочина","мм","189","189","189","","189"]
["","","","Височина","мм","295","295","295","","295"]
["Корпус","Colour","","","","Бяло","Бяло","Бяло","","Бяло"]
["Тегло","Тяло","","","кг","11.50","11.50","11.50","","11.50"]
["Вентилатор","Скорост на въздушния поток","Отопление","Висок","м³/мин","10.9","11.1","11.5","","15.1"]
["","","","Среден","м³/мин","8.7","9.0","9.0","","11.1"]
["","","","Ниско","м³/мин","6.4","6.4","6.4","","8.2"]
["","","","Тих режим","м³/мин","4.5","4.5","4.5","","5.7"]
["","","Охлаждане","Ниско","м³/мин","6.1","6.1","6.1","","7.6"]
["","","","Среден","м³/мин","8.2","8.6","8.6","","10.4"]
["","","","Висок","м³/мин","11.0","11.5","11.9","","13.5"]
["","","","Тих режим","м³/мин","4.6","4.6","4.6","","5.2"]
["Power supply","Phase","","","","1~","1~","1~","","1~"]
["","Име","","","","V1","V1","V1","","V1"]
["","Честота","","","Хц","50","50","50","","50"]
["","Напрежение","","","V","220-240","220-240","220-240","","220-240"]
["Входяща мощност","Охлаждане","","Ном.","kW","","","","0.028"]
["","Отопление","","Ном.","kW","","","","0.036"]
["Корпус","Цвят","","","","","","","Бяло"]
["Размери","Тяло","","Височина","мм","","","","295"]
["","","","Широчина","мм","","","","798"]
["","","","Дълбочина","мм","","","","189"]
["Тегло","Тяло","","","кг","","","","11.50"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","","","","13.1"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","","","","9.8"]
["","","","Ниско","м³/мин","","","","7.2"]
["","","","Тих режим","м³/мин","","","","4.6"]
["","","Отопление","Висок","м³/мин","","","","14.6"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","","","","10.5"]
["","","Отопление","Ниско","м³/мин","","","","7.7"]
["","","","Вентилатор-=-Скорост на въздушния поток-=-Отопление-=-Тих режим-=-м³/мин","м³/мин","","","","5.2"]
["Звукова мощност","Охлаждане","","","дБА","","","","60"]
["Ниво на звуково налягане","Охлаждане","","Висок","дБА","","","","45"]
["","","","Среден","дБА","","","","37"]
["","","","Ниско","дБА","","","","29"]
["","","","Тих режим","дБА","","","","21"]
["","Отопление","","Висок","дБА","","","","45"]
["","","","Среден","дБА","","","","37"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","дБА","","","","29"]
["","","","Тих режим","дБА","","","","21"]
["Хладилен агент","Потенциал на глобално затопляне","","","","","","","675.0"]
["Тръбни съединения","Tечност","","Вън. д.","мм","","","","6.35"]
["","Газ","","Вън. д.","мм","","","","12.70"]
["","Дренаж","","","","","","","18"]
["Системи за управление","Инфрачервено дистанционно управление","","","","","","","ARC466A58"]
["","Жично дистанционно управление","","","","","","","BRC073"]
["Стандартни аксесоари","Installation manual","","","","","","","1"]
["","Screw cover","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","General safety precautions","","","","","","","1"]
["","Operation manual","","","","","","","1"]
["","Въздушен филтър","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Remote controller mounting plate","","","","","","","1"]
["","Screw bag","","","","","","","1"]
["Електрозахранване","Име","","","","","","","V1"]
["","Фаза","","","","","","","1~"]
["","Честота","","","Хц","","","","50"]
["","Напрежение","","","V","","","","220-240"]