{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-CW / RXA-B"]
[]
[]
[]
[]
["","","","","FTXA50C2V1BW / RXA50B5V1B"]
["Капацитет на охлаждане","Мин.","","кВт","1.70"]
["","Ном.","","кВт","5.00"]
["","Макс.","","кВт","5.30"]
["Топлинен капацитет","Мин.","","кВт","1.70"]
["","Ном.","","кВт","5.80"]
["","Макс.","","кВт","6.50"]
["Номинална ефективност","EER","","","3.68"]
["","COP","","","4.00"]
["","Годишен разход на енергия","","kWh","679"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","A"]
["","","Отопление","","A"]
["Охлаждане с конвекция","Клас на енергийна ефективност","","","A++"]
["","Капацитет","Pdesign","кВт","5.00"]
["","SEER","","","7.33"]
["","Годишно потребление на електроенергия","","kWh/a","239"]
["Отопление с конвекция (умерен климат)","Клас на енергийна ефективност","","","A++"]
["","Капацитет","Pdesign","кВт","4.00"]
["","SCOP/A","","","4.60"]
["","Pdh Капацитет на отопление при -10°","","кВт","3.19"]
["","Годишно потребление на електроенергия","","kWh/a","1218"]