{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":11,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXC-E"]
[]
[]
[]
[]
["","","","","","FTXC20EV1B","FTXC25EV1B","FTXC35EV1B","FTXC50EV1B","FTXC60EV1B","FTXC71EV1B"]
["Входяща мощност","Охлаждане","","Ном.","кВт","0.595","0.765","1.045","1.55","1.89","2.38"]
["","Отопление","","Ном.","кВт","0.67","0.75","1.07","1.515","1.68","2.46"]
["Корпус","Цвят","","","","Бяло","Бяло","Бяло","Бяло","Бяло","Бяло"]
["","Материал","","","","Високоударен полистирол","Високоударен полистирол","Високоударен полистирол","Високоударен полистирол","Високоударен полистирол","Високоударен полистирол"]
["Размери","Тяло","","Височина","mm","288","288","288","288","297","297"]
["","","","Широчина","mm","770","770","770","770","990","990"]
["","","","Дълбочина","mm","234","234","234","234","273","273"]
["Тегло","Тяло","","","кг","9.0","9.0","9.5","9.5","13.0","13.0"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","10.8","10.8","11.1","12.5","20.4","20.4"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","8.1","8.1","8.7","9.9","14.5","14.5"]
["","","","Ниско","м³/мин","6.1","6.1","6.4","8.1","12.5","12.5"]
["","","","Тих режим","м³/мин","5.4","5.4","5.4","7.4","10.2","10.2"]
["Звукова мощност","Охлаждане","","","dBA","57","57","58","60","63","63"]
["Ниво на звуково налягане","Охлаждане","","Висок","dBA","40","40","41","47","48","48"]
["","","","Среден","dBA","33","33","34","39","42","42"]
["","","","Ниско","dBA","26","26","26","33","38","38"]
["","","","Тих режим","dBA","21","21","22","30","31","31"]
["Тръбни съединения","Tечност","","Вън. д.","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Газ","","Вън. д.","mm","9.52","9.52","9.52","12.7","12.7","12.7"]
["","Дренаж","","","","16.5","16.5","16.5","16.5","16.5","16.5"]
["Системи за управление","Инфрачервено дистанционно управление","","","","ARC486A6","ARC486A6","ARC486A6","ARC486A6","ARC486A6","ARC486A6"]
["Диапазон на енергийна ефективност","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Електрозахранване","Име","","","","V1","V1","V1","V1","V1","V1"]
["","Фаза","","","","1~","1~","1~","1~","1~","1~"]
["","Честота","","","Хц","50","50","50","50","50","50"]
["","Напрежение","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]