{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B","FTXF25B5V1B"]
["Ниво на звуково налягане","Отопление","Висок","dBA","39","40"]
["","","Среден","dBA","34","34"]
["","","Тих режим","dBA","21","21"]
["","","Ниско","dBA","28","28"]
["","Охлаждане","Среден","dBA","33","33"]
["","","Тих режим","dBA","20","20"]
["","","Ниско","dBA","25","26"]
["","","Висок","dBA","39","40"]
["Стандартни аксесоари","Ръководство за монтаж","","","1","1"]
["","Ръководство за работа","","","1","1"]
["","Инфрачервено дистанционно","","","1","1"]
["","Сухи батерии тип ААА","","","2","2"]
["","Стойка за дистанционното","","","1","1"]
["","Монтажна пластина:","","","1","1"]
["","Фиксиращи винтове за вътрешното устройство","","","2","2"]
["Системи за управление","Wired remote control","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","ARC470A1","ARC470A1"]
["Тръбни съединения","Tечност","Вън. д.","мм","6.35","6.35"]
["","Газ","Вън. д.","мм","9.50","9.50"]
["","Дренаж","","","18","18"]
["Консумирана мощност","Охлаждане","Ном.","кВт","0.017","0.019"]
["","Отопление","Ном.","кВт","0.020","0.020"]
["Sound power level","Охлаждане","","dBA","55","55"]
["","Отопление","","dBA","55","55"]
["Размери","Тяло","Широчина","мм","770","770"]
["","","Дълбочина","мм","225","225"]
["","","Височина","мм","286","286"]
["Корпус","Цвят","","","Бяло","Бяло"]
["Тегло","Тяло","","кг","8.50","8.50"]
["Power supply","Фаза","","","1~","1~"]
["","Честота","","Хц","50","50"]
["","Напрежение","","V","220-240","220-240"]