{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":90,"n_cols":12,"rows_kept":90,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-D"]
[]
[]
[]
[]
["","","","","","FTXF20D5V1B","FTXF25D5V1B","FTXF35D5V1B","FTXF42D5V1B","FTXF50D2V1B","FTXF60D2V1B","FTXF71D2V1B"]
["Входяща мощност","Охлаждане","","Ном.","кВт","","","","","0.029","","0.032"]
["","Отопление","","Ном.","кВт","","","","","0.032","","0.035"]
["Корпус","Colour","","","","","","","","Бяло","","Бяло"]
["Размери","Тяло","","Височина","mm","","","","","295","","295"]
["","","","Широчина","mm","","","","","990","","990"]
["","","","Дълбочина","mm","","","","","263","","263"]
["Тегло","Тяло","","","kg","","","","","13.5","","13.5"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","","","","","16.8","","17.3"]
["","","","Среден","м³/мин","","","","","14.4","","14.8"]
["","","","Ниско","м³/мин","","","","","11.9","","12.2"]
["","","","Тих режим","м³/мин","","","","","10.5","","10.7"]
["","","Отопление","Висок","м³/мин","","","","","17.3","","17.9"]
["","","","Среден","м³/мин","","","","","14.8","","15.8"]
["","","","Ниско","м³/мин","","","","","12.2","","12.8"]
["","","","Тих режим","м³/мин","","","","","10.7","","11.3"]
["Звукова мощност","Охлаждане","","","dBA","","","","","59","","62"]
["","Отопление","","","dBA","","","","","61","","62"]
["Ниво на звуково налягане","Охлаждане","","Висок","dBA","","","","","43","","46"]
["","","","Среден","dBA","","","","","39","","42"]
["","","","Ниско","dBA","","","","","34","","37"]
["","","","Тих режим","dBA","","","","","31","","34"]
["","Отопление","","Висок","dBA","","","","","42","","45"]
["","","","Среден","dBA","","","","","38","","41"]
["","","","Ниско","dBA","","","","","33","","36"]
["","","","Тих режим","dBA","","","","","30","","33"]
["Тръбни съединения","Tечност","","Вън. д.","mm","","","","","6.35","","6.35"]
["","Газ","","Вън. д.","mm","","","","","12.7","","12.7"]
["","Дренаж","","","","","","","","18","","18"]
["Control systems","Infrared remote control","","","","","","","","ARC470A1","","ARC470A1"]
["","Wired remote control","","","","","","","","BRC073A1","","BRC073A1"]
["Стандартни аксесоари","Сухи батерии тип ААА","","","","","","","","2","","2"]
["","Ръководство за монтаж","","","","","","","","1","","1"]
["","Ръководство за работа","","","","","","","","1","","1"]
["","Инфрачервено дистанционно","","","","","","","","1","","1"]
["","Стойка за дистанционното","","","","","","","","1","","1"]
["","Монтажна пластина:","","","","","","","","1","","1"]
["","Фиксиращи винтове за вътрешното устройство","","","","","","","","2","","2"]
["Power supply","Име","","","","","","","","V1","","V1"]
["","Phase","","","","","","","","1~","","1~"]
["","Честота","","","Хц","","","","","50","","50"]
["","Напрежение","","","V","","","","","220-240","","220-240"]
["Входяща мощност","Охлаждане","","Ном.","кВт","0.023","0.023","0.029","0.040","","0.032"]
["","Отопление","","Ном.","кВт","0.023","0.023","0.029","0.040","","0.035"]
["Корпус","Цвят","","","","Бяло","Бяло","Бяло","Бяло","","Бяло"]
["Размери","Тяло","","Височина","mm","286","286","286","286","","295"]
["","","","Широчина","mm","770","770","770","770","","990"]
["","","","Дълбочина","mm","225","225","225","225","","263"]
["Тегло","Тяло","","","kg","8","8","8.5","9.00","","13.5"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","9.8","10","11.5","12.6","","17.3"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","8","8","8","9","","14.8"]
["","","","Ниско","м³/мин","6","6.2","6.4","6.9","","12.2"]
["","","","Тих режим","м³/мин","4.3","4.3","4.4","4.9","","10.7"]
["","","Отопление","Висок","м³/мин","10.4","10.4","11.9","12.8","","17.9"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","8.3","8.4","8.6","8.8","","15.8"]
["","","Отопление","Ниско","м³/мин","6.2","6.4","6.5","6.7","","12.8"]
["","","","Вентилатор-=-Скорост на въздушния поток-=-Отопление-=-Тих режим-=-м³/мин","м³/мин","5.3","5.3","5.3","5.2","","11.3"]
["Звукова мощност","Охлаждане","","","dBA","53","54","54","59.0","","60"]
["","Отопление","","","dBA","55","55","56","59.0","","62"]
["Ниво на звуково налягане","Охлаждане","","Висок","dBA","39","40","43","45.0","","45"]
["","","","Среден","dBA","33","33","34","36.0","","41"]
["","","","Ниско","dBA","25","26","27","30.0","","36"]
["","","","Тих режим","dBA","20","20","20","22.0","","33"]
["","Отопление","","Висок","dBA","39","40","40","44.0","","44"]
["","","","Среден","dBA","34","34","35","34.0","","40"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","dBA","28","28","29","28.0","","35"]
["","","","Тих режим","dBA","21","21","21","22.0","","32"]
["Тръбни съединения","Tечност","","Вън. д.","mm","6","6","6","6","","6.35"]
["","Газ","","Вън. д.","mm","9.5","9.5","9.5","9.50","","12.7"]
["","Дренаж","","","","18","18","18","18","","18"]
["Системи за управление","Инфрачервено дистанционно управление","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1","","ARC470A1"]
["","Жично дистанционно управление","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","","BRC073A1"]
["Стандартни аксесоари","Installation manual","","","","1","1","1","1","","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","","2"]
["","General safety precautions","","","","196","196","196","196"]
["","Operation manual","","","","1","1","1","1","","1"]
["","Batteries","","","","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","","2"]
["","Infrared remote control","","","","1","1","1","1","","1"]
["","Mounting plate","","","","1","1","1","1","","1"]
["","Remote control holder","","","","1","1","1","1","","1"]
["Електрозахранване","Фаза","","","","1~","1~","1~","1~","","1~"]
["","Честота","","","Хц","50","50","50","50","","50"]
["","Напрежение","","","V","220-440","220-440","220-440","220-440","","220-240"]
["","Име","","","","","","","","","V1"]