{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":10,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS / 3MXM-N"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM40N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM40N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM52N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM52N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM68N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM68N2V1B"]
["Капацитет на охлаждане","Ном.","","kW","4.00","","4.00","5.20","4.00","6.00"]
["Номинална ефективност","Годишен разход на енергия","","kWh","467","","471","593","457","787"]
["","EER","","","4.28","","4.25","4.38","4.38","3.81"]
["","COP","","","4.32","","4.05","4.42","4.04","3.88"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","A","","A","A","A","A"]
["","","Отопление","","A","","A","A","A","A"]
["Топлинен капацитет","Ном.","","kW","4.60","","6.80","6.80","6.50","7.80"]
["Капацитет на охлаждане","Ном.","","kW","","4.00"]
["Топлинен капацитет","Ном.","","kW","","4.60"]
["Номинална ефективност","EER","","","","4.15"]
["","COP","","","","3.95"]
["","Годишен разход на енергия","","kWh","","482"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","","A"]
["","","Отопление","","","A"]
["Охлаждане с конвекция","Клас на енергийна ефективност","","","","A++"]
["","Капацитет","Pdesign","kW","","4.00"]
["","SEER","","","","7.62"]
["","Годишно потребление на електроенергия","","kWh/a","","164"]
["Отопление с конвекция (умерен климат)","Клас на енергийна ефективност","","","","A+"]
["","Капацитет","Pdesign","kW","","4.80"]
["","SCOP/A","","","","4.11"]
["","Pdh Капацитет на отопление при -10°","","kW","","3.58"]
["","Годишно потребление на електроенергия","","kWh/a","","1632"]
["Забележки","","","","","(1) - Номиналният капацитет на охлаждане се базира на: вътрешна темп.: 27°CDB, 19°CWB, външна температура: 35°CDB, еквивалентна дължина на тръбите за хладилен агент: 5 m, разлика в нивото: 0m."]
["","","","","","(2) - Номиналният капацитет за загряване важи за: вътрешна температура: 20°C (сух термометър), външна температура: 7°C (сух термометър), 8°C (влажен термометър), съответна дължина на тръбите: 5 м, денивелация: 0m."]
["","","","","","(3) - Вж. отделния чертеж за работен диапазон"]
["","","","","","(4) - Вж. отделния чертеж за електрическите схеми"]