{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":12,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G"]
[]
[]
[]
[]
["","","","","","FTXS20G2V1B","FTXS25G2V1B","FTXS35G2V1B","FTXS42G2V1B","FTXS50G2V1B","FTXS60GV1B","FTXS71GV1B"]
["Ниво на звуково налягане","Отопление","","Висок","dBA","38","39","42","42","44","","46"]
["","","","Тих режим","dBA","25","25","26","30","31","","34"]
["","","","Ниско","dBA","28","28","29","33","34","","37"]
["","Охлаждане","","Тих режим","dBA","22","22","23","30","31","","34"]
["","","","Ниско","dBA","25","25","26","33","34","","37"]
["","","","Висок","dBA","38","38","42","42","43","","46"]
["","","","Ном.","dBA","33","34","36","38","39","","42"]
["","Охлаждане","","Ном.","dBA","32","32","34","38","39","","42"]
["Стандартни аксесоари","Филтър за фотокаталитично пречистване на въздуха от титанов апатит","","","","2","2","2","2","2"]
["","Ръководство за работа","","","","1","1","1","1","1","","1"]
["","Ръководство за монтаж","","","","1","1","1","1","1","","1"]
["","Безжично дистанционно управление","","","","1","1","1","1","1","","1"]
["","Батерии","","","","2","2","2","2","2","","2"]
["","Стойка за дистанционното","","","","1","1","1","1","1","","1"]
["","Фиксиращи винтове за вътрешното устройство","","","","2","2","2","2","2","","2"]
["","Монтажна пластина:","","","","1","1","1","1","1","","1"]
["Системи за управление","Infrared remote control","","","","","","","","","","ARC452A3"]
["Тръбни съединения","Tечност","","Вън. д.","мм","6.35","6.35","6.35","6.35","6.35","","6.35"]
["","Газ","","Вън. д.","мм","9.52","9.52","9.52","9.52","12.70","","15.9"]
["","Дренаж","","","","18","18","18","18","18","","18"]
["Входяща мощност","Охлаждане","","Ном.","кВт","","","","","","","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Отопление","","Ном.","кВт","","","","","","","0.060 (2), 0.060 (3), 0.060 (4)"]
["Ниво на звукова мощност","Охлаждане","","","dBA","54","54","58","58","59","","63"]
["","Отопление","","","dBA","54","55","58","58","60","","62"]
["Размери","Тяло","","Широчина","мм","800","800","800","800","800","","1,050"]
["","","","Дълбочина","мм","215","215","215","215","215","","250"]
["","","","Височина","мм","295","295","295","295","295","","290"]
["Корпус","Цвят","","","","Бяло","Бяло","Бяло","Бяло","Бяло","","Бяло"]
["Тегло","Тяло","","","kg","9","9","10","10","10","","12"]
["Power supply","Фаза","","","","1~","1~","1~","1~","1~","","1~"]
["","Честота","","","Хц","50","50","50","50","50","","50"]
["","Име","","","","V1","V1","V1","V1","V1","","V1"]
["","Напрежение","","","V","220-240","220-240","220-240","220-240","220-240","","220-240"]
["Забележки","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - SL: Настройка за тихо ниво на темпото на въздушен поток"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Ном.","м³/мин","","","","","","16.0"]
["Ниво на звуково налягане","Охлаждане","","Ном.","dBA","","","","","","41"]
["Вентилатор","Скорост на въздушния поток","Отопление","Ном.","м³/мин","","","","","","14.9"]
["Ниво на звуково налягане","Отопление","","Ном.","dBA","","","","","","40"]
["Входяща мощност","Охлаждане","","Ном.","кВт","","","","","","0.040 (4) (2) (3), 0.040 (4) (2) (3), 0.040 (4) (2) (3)"]
["","Отопление","","Ном.","кВт","","","","","","0.045 (4) (2) (3), 0.045 (4) (2) (3), 0.045 (4) (2) (3)"]
["Корпус","Цвят","","","","","","","","","Бяло"]
["Размери","Тяло","","Височина","мм","","","","","","290"]
["","","","Широчина","мм","","","","","","1050"]
["","","","Дълбочина","мм","","","","","","250"]
["Тегло","Тяло","","","kg","","","","","","12"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","","","","","","16.0"]
["","","","Ниско","м³/мин","","","","","","11.3"]
["","","","Тих режим","м³/мин","","","","","","10.1"]
["","","Отопление","Висок","м³/мин","","","","","","17.2"]
["","","","Ниско","м³/мин","","","","","","12.6"]
["","","","Вентилатор-=-Скорост на въздушния поток-=-Отопление-=-Тих режим-=-м³/мин","м³/мин","","","","","","11.3"]
["Звукова мощност","Охлаждане","","","dBA","","","","","","60"]
["","Отопление","","","dBA","","","","","","59"]
["Ниво на звуково налягане","Охлаждане","","Висок","dBA","","","","","","45"]
["","","","Ниско","dBA","","","","","","36"]
["","","","Тих режим","dBA","","","","","","33"]
["","Отопление","","Висок","dBA","","","","","","44"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","dBA","","","","","","35"]
["","","","Тих режим","dBA","","","","","","32"]
["Тръбни съединения","Tечност","","Вън. д.","мм","","","","","","6.35"]
["","Газ","","Вън. д.","мм","","","","","","12.7"]
["","Дренаж","","","","","","","","","18"]
["Системи за управление","Инфрачервено дистанционно управление","","","","","","","","","ARC452A3"]
["Стандартни аксесоари","Installation manual","","","","","","","","","1"]
["","Wireless remote control","","","","","","","","","1"]
["","Operation manual","","","","","","","","","1"]
["","Batteries","","","","","","","","","2"]
["","Indoor unit fixing screws","","","","","","","","","2"]
["","Mounting plate","","","","","","","","","1"]
["","Remote control holder","","","","","","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","","","","","","2"]
["Електрозахранване","Име","","","","","","","","","V1"]
["","Фаза","","","","","","","","","1~"]
["","Честота","","","Хц","","","","","","50"]
["","Напрежение","","","V","","","","","","220-240"]
["Стандартни аксесоари","Филтър за фотокаталитично пречистване на въздуха от титанов апатит без рамка","","","","","","","","","","2"]
["Забележки","","","","","","","","","","","(4) - 240V"]