{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":5,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-AW"]
[]
[]
[]
[]
["","","","","FTXTA30A2V1BW"]
["Ниво на звуково налягане","Отопление","Висок","dBA","41"]
["","","Среден","dBA","31"]
["","","Тих режим","dBA","19"]
["","","Ниско","dBA","24"]
["","Охлаждане","Среден","dBA","32"]
["","","Тих режим","dBA","20"]
["","","Ниско","dBA","25"]
["","","Висок","dBA","43"]
["Стандартни аксесоари","Ръководство за монтаж","","","1"]
["","Ръководство за работа","","","1"]
["","Въздушен филтър","","","2"]
["","Инфрачервено дистанционно","","","1"]
["","Монтажна пластина за дистанционно","","","1"]
["","Плик за винтове","","","1"]
["","Винтов капак","","","2"]
["","Сухи батерии тип ААА","","","2"]
["","Общи мерки за безопасност","","","1"]
["Хладилен агент","Потенциал на глобално затопляне","","","675.0"]
["Control systems","Wired remote control","","","BRC073A4"]
["","Infrared remote control","","","ARC466A59"]
["Тръбни съединения","Tечност","Вън. д.","mm","6.35"]
["","Газ","Вън. д.","mm","9.50"]
["","Дренаж","","","18"]
["Входяща мощност","Охлаждане","Ном.","кВт","0.023"]
["","Отопление","Ном.","кВт","0.022"]
["Звукова мощност","Охлаждане","","dBA","60"]
["","Отопление","","dBA","60"]
["Размери","Тяло","Широчина","mm","798"]
["","","Дълбочина","mm","189"]
["","","Височина","mm","295"]
["Корпус","Colour","","","Бяло"]
["Тегло","Тяло","","kg","11.5"]
["Power supply","Phase","","","1~"]
["","Честота","","Хц","50"]
["","Име","","","V1"]
["","Напрежение","","V","220-240"]