{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-BB"]
[]
[]
[]
[]
["","","","","","FTXTA30B2V1BB"]
["Ниво на звуково налягане","Отопление","","Висок","dBA","41"]
["","","","Среден","dBA","31"]
["","","","Тих режим","dBA","19"]
["","","","Ниско","dBA","24"]
["","Охлаждане","","Среден","dBA","32"]
["","","","Тих режим","dBA","20"]
["","","","Ниско","dBA","25"]
["","","","Висок","dBA","43"]
["Стандартни аксесоари","Ръководство за монтаж","","","","1"]
["","Ръководство за работа","","","","1"]
["","Въздушен филтър","","","","2"]
["","Инфрачервено дистанционно","","","","1"]
["","Монтажна пластина за дистанционно","","","","1"]
["","Плик за винтове","","","","1"]
["","Винтов капак","","","","2"]
["","Сухи батерии тип ААА","","","","2"]
["","Общи мерки за безопасност","","","","1"]
["Хладилен агент","Потенциал на глобално затопляне","","","","675.0"]
["Системи за управление","Wired remote control","","","","BRC073A4"]
["","Infrared remote control","","","","ARC466A59"]
["Тръбни съединения","Tечност","","Вън. д.","мм","6.35"]
["","Газ","","Вън. д.","мм","9.50"]
["","Дренаж","","","","18"]
["Консумирана мощност","Охлаждане","","Ном.","кВт","0.023"]
["","Отопление","","Ном.","кВт","0.022"]
["Sound power level","Охлаждане","","","dBA","60"]
["","Отопление","","","dBA","60"]
["Размери","Тяло","","Широчина","мм","798"]
["","","","Дълбочина","мм","189"]
["","","","Височина","мм","295"]
["Корпус","Colour","","","","Черно"]
["Тегло","Тяло","","","кг","11.5"]
["Fan","Скорост на въздушния поток","Отопление","Висок","м³/мин","11.5"]
["","","","Ниско","м³/мин","6.0"]
["","","","Среден","м³/мин","8.0"]
["","","","Тих режим","м³/мин","5.1"]
["","","Охлаждане","Ниско","м³/мин","5.7"]
["","","","Среден","м³/мин","8.3"]
["","","","Висок","м³/мин","11.9"]
["","","","Тих режим","м³/мин","4.6"]
["Power supply","Phase","","","","1~"]
["","Честота","","","Хц","50"]
["","Име","","","","V1"]
["","Напрежение","","","V","220-240"]
["Забележки","","","","","(1) - Охлаждане: температура на открито 27°C със сух термометър, 19.0°C с влажен термометър; външна темп. 35°C със сух термометър; 24°C с влажен термометър; съответстваща дължина на тръбопр.: 5м"]
["","","","","","(2) - Отопление: температура на открито 20°С (сух термометър), външна темп. 7°C (сух термометър), 6°C (влажен термометър); съответна дължина на тръбите за хладилния агент: 5м"]
["","","","","","(3) - Вж. отделния чертеж за електрическите схеми"]