{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":6,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-CW"]
[]
[]
[]
[]
["","","","","","FTXTA30C2V1BW"]
["Входяща мощност","Охлаждане","","Ном.","кВт","0.023"]
["","Отопление","","Ном.","кВт","0.022"]
["Корпус","Цвят","","","","Бяло"]
["Размери","Тяло","","Височина","mm","295"]
["","","","Широчина","mm","798"]
["","","","Дълбочина","mm","189"]
["Тегло","Тяло","","","kg","12"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","13.1"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","9"]
["","","","Ниско","м³/мин","6"]
["","","","Тих режим","м³/мин","4.9"]
["","","Отопление","Висок","м³/мин","12.3"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","8.2"]
["","","Отопление","Ниско","м³/мин","5.8"]
["","","","Вентилатор-=-Скорост на въздушния поток-=-Отопление-=-Тих режим-=-м³/мин","м³/мин","5"]
["Звукова мощност","Охлаждане","","","dBA","60"]
["","Отопление","","","dBA","60"]
["Ниво на звуково налягане","Охлаждане","","Висок","dBA","43"]
["","","","Среден","dBA","32"]
["","","","Ниско","dBA","25"]
["","","","Тих режим","dBA","20"]
["","Отопление","","Висок","dBA","41"]
["","","","Среден","dBA","31"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","dBA","24"]
["","","","Тих режим","dBA","19"]
["Хладилен агент","Потенциал на глобално затопляне","","","","675"]
["Тръбни съединения","Tечност","","Вън. д.","mm","6.35"]
["","Газ","","Вън. д.","mm","9.5"]
["","Дренаж","","","","18"]
["Control systems","Infrared remote control","","","","ARC466A84"]
["Системи за управление","Жично дистанционно управление","","","","BRC073A4"]
["Стандартни аксесоари","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Електрозахранване","Фаза","","","","1~"]
["","Честота","","","Хц","50"]
["","Напрежение","","","V","220-240"]