{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-M"]
[]
[]
[]
[]
["","","","","","FTXTM30M2V1B","FTXTM40M2V1B"]
["Входяща мощност","Охлаждане","","Ном.","kW","0.032","0.037"]
["","Отопление","","Ном.","kW","0.037","0.04"]
["Корпус","Цвят","","","","Бяло","Бяло"]
["Размери","Тяло","","Височина","мм","294","300"]
["","","","Широчина","мм","811","1040"]
["","","","Дълбочина","мм","272","295"]
["Тегло","Тяло","","","kg","10","14.5"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","11.7","15.5"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","8","9.2"]
["","","","Ниско","м³/мин","6.3","5.7"]
["","","","Тих режим","м³/мин","5.2","4.6"]
["","","Отопление","Висок","м³/мин","12.2","17.7"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","7.5","11"]
["","","Отопление","Ниско","м³/мин","5.1","7.5"]
["","","","Вентилатор-=-Скорост на въздушния поток-=-Отопление-=-Тих режим-=-м³/мин","м³/мин","4.1","6.3"]
["Звукова мощност","Охлаждане","","","дБА","60","60"]
["","Отопление","","","дБА","61","61"]
["Ниво на звуково налягане","Охлаждане","","Висок","дБА","45","46"]
["","","","Среден","дБА","33","32"]
["","","","Ниско","дБА","25","24"]
["","","","Тих режим","дБА","21","20"]
["","Отопление","","Висок","дБА","45","46"]
["","","","Среден","дБА","31","31"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","дБА","22","22"]
["","","","Тих режим","дБА","19","19"]
["Тръбни съединения","Tечност","","Вън. д.","мм","6.35","6.35"]
["","Газ","","Вън. д.","мм","9.5","9.5"]
["","Дренаж","","","","16 (iвътрешен диаметър на свързващ маркуч)","16 (iвътрешен диаметър на свързващ маркуч)"]
["Системи за управление","Инфрачервено дистанционно управление","","","","ARC466A55","ARC466A55"]
["","Жично дистанционно управление","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Електрозахранване","Име","","","","V1","V1"]
["","Фаза","","","","1~","1~"]
["","Честота","","","Хц","50","50"]
["","Напрежение","","","V","220-240","220-240"]