{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":7,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-S"]
[]
[]
[]
[]
["","","","","","FTXTM30S2V1B","FTXTM40S2V1B"]
["Входяща мощност","Охлаждане","","Ном.","кВт","0.035","0.053"]
["","Отопление","","Ном.","кВт","0.039","0.06"]
["Корпус","Цвят","","","","Бяло","Бяло"]
["Размери","Тяло","","Височина","mm","295","299"]
["","","","Широчина","mm","778","998"]
["","","","Дълбочина","mm","272","292"]
["Тегло","Тяло","","","kg","10","15"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","11.5","15.1"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","7.5","9.2"]
["","","","Ниско","м³/мин","5.2","5.6"]
["","","","Тих режим","м³/мин","4.2","4.8"]
["","","Отопление","Висок","м³/мин","11.6","17"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","7.3","10"]
["","","Отопление","Ниско","м³/мин","4.7","6"]
["","","","Вентилатор-=-Скорост на въздушния поток-=-Отопление-=-Тих режим-=-м³/мин","м³/мин","4","5.1"]
["Звукова мощност","Охлаждане","","","dBA","60","60"]
["","Отопление","","","dBA","60","60"]
["Ниво на звуково налягане","Охлаждане","","Висок","dBA","45","46"]
["","","","Среден","dBA","33","32"]
["","","","Ниско","dBA","25","24"]
["","","","Тих режим","dBA","21","20"]
["","Отопление","","Висок","dBA","45","46"]
["","","","Среден","dBA","31","31"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","dBA","22","22"]
["","","","Тих режим","dBA","19","19"]
["Хладилен агент","Потенциал на глобално затопляне","","","","675","675"]
["Тръбни съединения","Tечност","","Вън. д.","mm","6.35","6.35"]
["","Газ","","Вън. д.","mm","9.5","9.5"]
["","Дренаж","","","","18","18"]
["Системи за управление","Инфрачервено дистанционно управление","","","","ARC466A83","ARC466A83"]
["","Жично дистанционно управление","","","","BRC073A1","BRC073A1"]
["Стандартни аксесоари","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Електрозахранване","Фаза","","","","1~","1~"]
["","Честота","","","Хц","50","50"]
["","Напрежение","","","V","220-240","220-240"]