{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":83,"n_cols":7,"rows_kept":83,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Ниво на звуково налягане","Отопление","","Висок","дБА","43"]
["","","","Среден","дБА","35"]
["","","","Тих режим","дБА","21"]
["","","","Ниско","дБА","26"]
["","Охлаждане","","Среден","дБА","35"]
["","","","Тих режим","дБА","21"]
["","","","Ниско","дБА","26"]
["","","","Висок","дБА","43"]
["Стандартни аксесоари","Ръководство за монтаж","","","","1"]
["","Ръководство за работа","","","","1"]
["","Безжично дистанционно управление","","","","1"]
["","Сухи батерии тип ААА","","","","2"]
["","Стойка за дистанционното","","","","1"]
["","Монтажна пластина:","","","","1"]
["","Обезмирисяващ филтър с титанов апатит","","","","2"]
["","Фиксиращи винтове за вътрешното устройство","","","","2"]
["Системи за управление","Жично дистанционно управление","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A11"]
["Тръбни връзки","Tечност","","Вън. д.","мм","6.35"]
["","Газ","","Вън. д.","мм","9.50"]
["","Дренаж","","","","16 (iвътрешен диаметър на свързващ маркуч)"]
["Power input","Охлаждане","","Ном.","kW","0.030"]
["","Отопление","","Ном.","kW","0.035"]
["Sound power level","Охлаждане","","","дБА","58"]
["","Отопление","","","дБА","58"]
["Размери","Тяло","","Широчина","мм","770"]
["","","","Дълбочина","мм","225"]
["","","","Височина","мм","285"]
["Корпус","Цвят","","","","Бяло"]
["Тегло","Тяло","","","kg","9.0"]
["Power supply","Фаза","","","","1~"]
["","Честота","","","Хц","50"]
["","Име","","","","V1"]
["","Напрежение","","","V","220-240"]
["Забележки","","","","","(1) - Вж. отделния чертеж за електрическите схеми"]
["Входяща мощност","Охлаждане","","Ном.","kW","","0.03"]
["","Отопление","","Ном.","kW","","0.035"]
["Корпус","Цвят","","","","","Бяло"]
["Размери","Тяло","","Височина","мм","","285"]
["","","","Широчина","мм","","770"]
["","","","Дълбочина","мм","","225"]
["Тегло","Тяло","","","kg","","9"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","","11.4"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","","8.2"]
["","","","Ниско","м³/мин","","5.4"]
["","","","Тих режим","м³/мин","","4.3"]
["","","Отопление","Висок","м³/мин","","10.8"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","","7.8"]
["","","Отопление","Ниско","м³/мин","","5.8"]
["","","","Вентилатор-=-Скорост на въздушния поток-=-Отопление-=-Тих режим-=-м³/мин","м³/мин","","4.9"]
["Звукова мощност","Охлаждане","","","дБА","","58"]
["","Отопление","","","дБА","","58"]
["Ниво на звуково налягане","Охлаждане","","Висок","дБА","","43"]
["","","","Среден","дБА","","35"]
["","","","Ниско","дБА","","26"]
["","","","Тих режим","дБА","","21"]
["","Отопление","","Висок","дБА","","43"]
["","","","Среден","дБА","","35"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","дБА","","26"]
["","","","Тих режим","дБА","","21"]
["Тръбни съединения","Tечност","","Вън. д.","мм","","6.35"]
["","Газ","","Вън. д.","мм","","9.5"]
["","Дренаж","","","","","16 (iвътрешен диаметър на свързващ маркуч)"]
["Системи за управление","Infrared remote control","","","","","ARC480A11"]
["Системи за управление","Жично дистанционно управление","","","","","BRC944B2, BRC073A1"]
["Стандартни аксесоари","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Електрозахранване","Име","","","","","V1"]
["","Фаза","","","","","1~"]
["","Честота","","","Хц","","50"]
["","Напрежение","","","V","","220-240"]