{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N"]
[]
[]
[]
[]
["","","","","","FTXZ25NV1B","FTXZ35NV1B","FTXZ50NV1B"]
["Ниво на звуково налягане","Отопление","","Висок","дБА","39","42","44"]
["","","","Тих режим","дБА","19","19","24"]
["","","","Ниско","дБА","28","29","31"]
["","Охлаждане","","Тих режим","дБА","19","19","23"]
["","","","Ниско","дБА","26","27","30"]
["","","","Висок","дБА","38","42","47"]
["","","","Ном.","дБА","35","36","38"]
["","Охлаждане","","Ном.","дБА","33","35","38"]
["Стандартни аксесоари","Фотокаталитичен филтър за пречистване и обезмирисяване на въздуха","","","","1","1","1"]
["","Безжично дистанционно управление","","","","1","1","1"]
["","Сухи батерии","","","","2","2","2"]
["","Стойка за дистанционното","","","","1","1","1"]
["","Фиксиращи винтове за вътрешното устройство","","","","3","3","3"]
["","Монтажна пластина:","","","","1","1","1"]
["Системи за управление","Infrared remote control","","","","ARC477A1","ARC477A1","ARC477A1"]
["Тръбни връзки","Tечност","","Вън. д.","мм","6.35","6.35","6.35"]
["","Газ","","Вън. д.","мм","9.5","9.5","9.5"]
["Power input","Охлаждане","","Ном.","kW","0.030","0.030","0.030"]
["","Отопление","","Ном.","kW","0.030","0.030","0.030"]
["Sound power level","Охлаждане","","","дБА","54","57","60"]
["","Отопление","","","дБА","56","57","59"]
["Размери","Тяло","","Широчина","мм","798","798","798"]
["","","","Дълбочина","мм","372","372","372"]
["","","","Височина","мм","295","295","295"]
["Корпус","Цвят","","","","Бяло","Бяло","Бяло"]
["Тегло","Тяло","","","kg","15","15","15"]
["Вентилатор","Скорост на въздушния поток","Отопление","Висок","м³/мин","11.7","13.3","14.4"]
["","","","Ниско","м³/мин","6.7","6.9","7.7"]
["","","","Тих режим","м³/мин","4.8","4.8","5.9"]
["","","Охлаждане","Ниско","м³/мин","5.3","5.6","6.6"]
["","","","Висок","м³/мин","10.7","12.1","15.0"]
["","","","Тих режим","м³/мин","4.0","4.0","4.6"]
["","","","Ном.","м³/мин","8.6","9.2","10.7"]
["","","Охлаждане","Ном.","м³/мин","7.5","8.4","9.2"]
["Power supply","Фаза","","","","1~","1~","1~"]
["","Име","","","","V1","V1","V1"]
["","Честота","","","Хц","50","50","50"]
["","Напрежение","","","V","220-240","220-240","220-240"]
["Забележки","","","","","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Предна част на топлообменника","(4) - Предна част на топлообменника","(4) - Предна част на топлообменника"]
["","","","","","(5) - Задна част на топлообменника","(5) - Задна част на топлообменника","(5) - Задна част на топлообменника"]