{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Ниво на звуково налягане","Отопление","","Висок","dBA","","","","41","46","47"]
["","","","Среден","dBA","","","","38","42","43"]
["","","","Ниско","dBA","","","","35","39","40"]
["","Охлаждане","","Среден","dBA","","","","38","42","43"]
["","","","Ниско","dBA","","","","35","39","40"]
["","","","Висок","dBA","","","","41","46","47"]
["Стандартни аксесоари","Ръководство за работа","","","","","","","1","1","1"]
["","Ръководство за монтаж","","","","","","","1","1","1"]
["","Маркуч за източване","","","","","","","1","1","1"]
["","Термоизолационна тръба","","","","","","","3","3","3"]
["","Заключващи се връзки","","","","","","","10","10","10"]
["","Лента за маркуч","","","","","","","1","1","1"]
["","Материал за уплътнение","","","","","","","4","4","4"]
["","Шайба за фиксиране на пластина","","","","","","","1","1","1"]
["","Съединение за източване","","","","","","","1","1","1"]
["","Нетъкана материя","","","","","","","1","1","1"]
["","Шайба","","","","","","","8","8","8"]
["","Фиксиращ винт за източващия маркуч","","","","","","","5","5","5"]
["Системи за управление","Wired remote control","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Капацитет на охлаждане","Общ капацитет","","Ном.","кВт","","","","","","12.1"]
["Тръбни съединения","Tечност","","Вън. д.","мм","","","","9.52","9.52","9.52"]
["","Газ","","Вън. д.","мм","","","","15.9","15.9","15.9"]
["","Дренаж","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Sound power level","Охлаждане","","","dBA","","","","59","64","65"]
["","Отопление","","","dBA","","","","59","64"]
["Размери","Тяло","","Широчина","мм","","","","950","950","950"]
["","","","Дълбочина","мм","","","","950","950","950"]
["","","","Височина","мм","","","","198","198","198"]
["Корпус","Материал","","","","","","","Смола","Смола","Смола"]
["","Цвят","","","","","","","Свежо бяло","Свежо бяло","Свежо бяло"]
["Тегло","Тяло","","","кг","","","","25.0","26.0","26"]
["Вентилатор","Скорост на въздушния поток","Отопление","Висок","м³/мин","","","","23.0","31.0","32.5"]
["","","","Среден","м³/мин","","","","19.5","25.5","26.5"]
["","","","Ниско","м³/мин","","","","16.0","20.0","20.5"]
["","","Охлаждане","Ниско","м³/мин","","","","16.0","20.0","20.5"]
["","","","Среден","м³/мин","","","","19.5","25.5","26.5"]
["","","","Висок","м³/мин","","","","23.0","31.0","32.5"]
["Височина за източване","мм","","","","","","","600","600","600"]
["Капацитет на отопление","Общ капацитет","","Ном.","кВт","","","","","","13.5"]
["Корпус","Цвят","","","","Свежо бяло","Свежо бяло","Свежо бяло"]
["","Материал","","","","Смола","Смола","Смола"]
["Размери","Тяло","","Височина","мм","198","198","198"]
["","","","Широчина","мм","950","950","950"]
["","","","Дълбочина","мм","950","950","950"]
["Тегло","Тяло","","","кг","25.0","26.0","26.0"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","23.0","31.0","32.5"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","19.5","25.5","26.5"]
["","","","Ниско","м³/мин","16.0","20.0","20.5"]
["","","Отопление","Висок","м³/мин","23.0","31.0","32.5"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","19.5","25.5","26.5"]
["","","Отопление","Ниско","м³/мин","16.0","20.0","20.5"]
["Звукова мощност","Охлаждане","","","dBA","59","64","65"]
["Ниво на звуково налягане","Охлаждане","","Висок","dBA","41","46","47"]
["","","","Среден","dBA","38","42","43"]
["","","","Ниско","dBA","35","39","40"]
["","Отопление","","Висок","dBA","41","46","47"]
["","","","Среден","dBA","38","42","43"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","dBA","35","39","40"]
["Тръбни съединения","Tечност","","Вън. д.","мм","9.52","9.52","9.52"]
["","Газ","","Вън. д.","мм","15.9","15.9","15.9"]
["","Дренаж","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Височина за източване","мм","","","","600","600","600"]
["Стандартни аксесоари","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Капацитет на охлаждане","Общ капацитет","","Ном.","кВт","","","12.10"]
["Капацитет на отопление","Общ капацитет","","Ном.","кВт","","","13.5"]