{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":9,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A"]
[]
[]
[]
[]
["","","","","","FVA71AMVEB","FVA100AMVEB","FVA125AMVEB","FVA140AMVEB"]
["Капацитет на охлаждане","Общ капацитет","","Ном.","кВт","","","12.10","13.40"]
["Капацитет на отопление","Общ капацитет","","Ном.","кВт","","","13.5","15.5"]
["Корпус","Цвят","","","","Свежо бяло","Свежо бяло","Свежо бяло","Свежо бяло"]
["Размери","Тяло","","Височина","мм","1850","1850","1850","1850"]
["","","","Широчина","мм","600","600","600","600"]
["","","","Дълбочина","мм","270","350","350","350"]
["Тегло","Тяло","","","кг","42","50","50","50"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","18","28","28","30"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","16","25","26","28"]
["","","","Ниско","м³/мин","14","22","24","26"]
["","","Отопление","Висок","м³/мин","18","28","28","30"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","16","25","26","28"]
["","","Отопление","Ниско","м³/мин","14","22","24","26"]
["Звукова мощност","Охлаждане","","","дБА","55","62","63","65"]
["Ниво на звуково налягане","Охлаждане","","Висок","дБА","43","50","51","53"]
["","","","Среден","дБА","41","47","48","51"]
["","","","Ниско","дБА","38","44","46","48"]
["","Отопление","","Висок","дБА","43","50","51","53"]
["","","","Среден","дБА","38","44","46","48"]
["","","","Ном.","дБА","41","47","48","51"]
["Тръбни съединения","Tечност","","Вън. д.","мм","9.52","9.52","9.52","9.52"]
["","Газ","","Вън. д.","мм","15.9","15.9","15.9","15.9"]
["","Дренаж","","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Системи за управление","Жично дистанционно управление","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Стандартни аксесоари","Installation manual","","","","1","1","1","1"]
["","Hole protection rubber","","","","2","2","2","2"]
["","Cover","","","","1","1","1","1"]
["","Dew proof material","","","","1","1","1","1"]
["","Remote control wiring","","","","1","1","1","1"]
["","Bracket for installation","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Bush","","","","1","1","1","1"]
["","Installation pattern","","","","1","1","1","1"]
["","Insulation for fitting for gas pipe","","","","1","1","1","1"]
["","Insulation for fitting for liquid pipe","","","","1","1","1","1"]
["","Screws","","","","5","5","5","5"]
["","Tie-wraps","","","","5","5","5","5"]
["Електрозахранване","Фаза","","","","1~","1~","1~","1~"]
["","Честота","","","Хц","50/60","50/60","50/60","50/60"]
["","Напрежение","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]