{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K / RXLG-M"]
[]
[]
[]
[]
["","","","","FVXG25K2V1B / RXLG25M2V1B","FVXG35K2V1B / RXLG35M2V1B"]
["Капацитет на охлаждане","Мин.","","кВт","1.2","1.4"]
["","Макс.","","кВт","5.1","5.6"]
["","Ном.","","кВт","2.5 (2)","3.5 (2)"]
["Тръбни съединения","Tечност","Вън. д.","мм","6.35","6.35"]
["","Газ","Вън. д.","мм","9.5","9.5"]
["","Дренаж","вън. д.","мм","18","18"]
["Номинална ефективност","Годишен разход на енергия","","kWh","355","510"]
["","EER","","","3.52 (1)","3.43 (1)"]
["","COP","","","3.88 (1)","3.61 (1)"]
["","Директива за обозначаване на енергийната ефективност:","Охлаждане","","A","A"]
["","","Отопление","","A","A"]
["Капацитет на отопление","Ном.","","кВт","4.5 (2)","5.6 (2)"]
["","Мин.","","кВт","1.0 (6)","1.1 (6)"]
["","Макс.","","кВт","6.5, 3.5 (7)","7.0, 4.0 (7)"]
["Забележки","","","","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС","(1) - EER/COP съгласно Eurovent 2012, за използване само извън ЕС"]
["","","","","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване","(2) - Номинална ефективност: охлаждане при 35°/27° номинално натоварване, отопление при 7°/20° номинално натоварване"]
["","","","","(3) - 220V","(3) - 220V"]
["","","","","(4) - 230V","(4) - 230V"]
["","","","","(5) - 240V","(5) - 240V"]
["","","","","(6) - За номиналния минимален капацитет, вентилаторът на вътр. тяло е настроен за SL кран","(6) - За номиналния минимален капацитет, вентилаторът на вътр. тяло е настроен за SL кран"]
["","","","","(7) - Максимален капацитет на отопление при външна температура -15°C","(7) - Максимален капацитет на отопление при външна температура -15°C"]