{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-A9"]
[]
[]
[]
[]
["","","","","","FVXM25A3V1B9","FVXM35A3V1B9","FVXM50A3V1B9"]
["Входяща мощност","Охлаждане","","Ном.","кВт","0.02","0.02","0.03"]
["","Отопление","","Ном.","кВт","0.02","0.03","0.03"]
["Корпус","Цвят","","","","Бяло","Бяло","Бяло"]
["Размери","Тяло","","Височина","мм","600","600","600"]
["","","","Широчина","мм","750","750","750"]
["","","","Дълбочина","мм","238","238","238"]
["Тегло","Тяло","","","кг","17","17","17"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","8.7","9.2","11.6"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","7","7","9"]
["","","","Ниско","м³/мин","4.9","4.9","6.6"]
["","","","Тих режим","м³/мин","4.1","4.1","5.4"]
["","","Отопление","Висок","м³/мин","9.2","9.8","12.8"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","7.2","7.2","10"]
["","","Отопление","Ниско","м³/мин","5.6","5.6","8.4"]
["","","","Вентилатор-=-Скорост на въздушния поток-=-Отопление-=-Тих режим-=-м³/мин","м³/мин","4.1","4.1","5.9"]
["Звукова мощност","Охлаждане","","","дБА","52","53","61"]
["","Отопление","","","дБА","52","53","62"]
["Ниво на звуково налягане","Охлаждане","","Висок","дБА","38","39","44"]
["","","","Среден","дБА","32","32","38"]
["","","","Ниско","дБА","25","25","31"]
["","","","Тих режим","дБА","20","20","27"]
["","Отопление","","Висок","дБА","38","39","46"]
["","","","Среден","дБА","32","32","40"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","дБА","25","25","35"]
["","","","Тих режим","дБА","19","19","29"]
["Хладилен агент","Потенциал на глобално затопляне","","","","675","675","675"]
["Тръбни съединения","Tечност","","Вън. д.","мм","6.4","6.4","6.4"]
["","Газ","","Вън. д.","мм","9.5","9.5","12.7"]
["","Дренаж","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Системи за управление","Инфрачервено дистанционно управление","","","","ARC466A66","ARC466A66","ARC466A66"]
["","Жично дистанционно управление","","","","BRC073A1","BRC073A1","BRC073A1"]
["Електрозахранване","Фаза","","","","1~","1~","1~"]
["","Честота","","","Хц","50","50","50"]
["","Напрежение","","","V","220-240","220-240","220-240"]
["Стандартни аксесоари","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Remote control holder","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]