{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":8,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-A9"]
[]
[]
[]
[]
["","","","","","RXA20A5V1B9","RXA25A5V1B9","RXA35A5V1B9"]
["Размери","Тяло","","Височина","мм","550","550","550"]
["","","","Широчина","мм","840","840","840"]
["","","","Дълбочина","мм","350","350","350"]
["Тегло","Тяло","","","kg","32","32","32"]
["Компресор","Тип","","","","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор"]
["Работен диапазон","Охлаждане","околна температура","Мин.","°C (сух термометър)","-10","-10","-10"]
["","","","Макс.","°C (сух термометър)","46","46","46"]
["","Отопление","околна температура","Мин.","°C с влажен термометър","-15","-15","-15"]
["","","","Макс.","°C с влажен термометър","18","18","18"]
["Ниво на звуково налягане","Охлаждане","","Ном.","дБА","46.0","46.0","49.0"]
["","Отопление","","Ном.","дБА","47.0","47.0","49.0"]
["Хладилен агент","Тип","","","","R-32","R-32","R-32"]
["","Зареждане","","","kg","0.76","0.76","0.76"]
["","Маса","","","tCO2Eq","0.52","0.52","0.52"]
["","Потенциал на глобално затопляне","","","","675.0","675.0","675.0"]
["Тръбни съединения","Дължина на тръбите","Макс.","Външ. у-во - Вътр. у-во","м","20","20","20"]
["","Допълнително количество хладилен агент","","","кг/м","0,02 (за дължина на тръбопровод, надвишаваща 10 м)","0,02 (за дължина на тръбопровод, надвишаваща 10 м)","0,02 (за дължина на тръбопровод, надвишаваща 10 м)"]
["","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","15.0","15.0","15.0"]
["Стандартни аксесоари","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["Електрозахранване","Фаза","","","","1~","1~","1~"]
["","Честота","","","Хц","50","50","50"]
["","Напрежение","","","V","220-240","220-240","220-240"]