{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":10,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXL-K"]
[]
[]
[]
[]
["","","","","","RXL20K3V1B","RXL25K3V1B","RXL35K2V1B","RXL42K2V1B","RXL50K2V1B"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Свръх ниска","м³/мин","","","30.1","30.6","48.9"]
["","","Отопление","Свръх ниска","м³/мин","","","25.6","27.2","43.1"]
["","","","Свръх ниска","cfm","","","1063","1080","1727"]
["","","Отопление","Свръх ниска","cfm","","","904","960","1522"]
["Размери","Тяло","","Височина","мм","550","550","550","550","735"]
["","","","Широчина","мм","765","765","765","765","825"]
["","","","Дълбочина","мм","285","285","285","285","300"]
["Тегло","Тяло","","","kg","34","34","34","39","47"]
["Електромотор на вентилатор","Скорост","Охлаждане","Свръх ниска","обор.","780","780","780","790","670"]
["","","Отопление","Свръх ниска","обор.","740","740","740","780","670"]
["Компресор","Тип","","","","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор"]
["Работен диапазон","Охлаждане","околна температура","Мин.","°C (сух термометър)","-10","-10","-10","-10","-10"]
["","","","Макс.","°C (сух термометър)","46","46","46","46","46"]
["","Отопление","околна температура","Мин.","°C с влажен термометър","-25","-25","-25","-25","-25"]
["","","","Макс.","°C с влажен термометър","18","18","18","18","18"]
["Ниво на звуково налягане","Охлаждане","","Висок","дБА","46","46","48","48","48"]
["","Отопление","","Висок","дБА","47","47","48","48","48"]
["Хладилен агент","Тип","","","","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Зареждане","","","kg","1.0","1.05","1.2","1.3","1.7"]
["","Маса","","","tCO2Eq","2.1","2.2","2.5","2.7","3.5"]
["","Потенциал на глобално затопляне","","","","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Тръбни съединения","Дължина на тръбите","Макс.","Външ. у-во - Вътр. у-во","м","20","20","20","20","30"]
["","Допълнително количество хладилен агент","","","кг/м","0,02 (за дължина на тръбопровод, надвишаваща 10 м)","0,02 (за дължина на тръбопровод, надвишаваща 10 м)","0,02 (за дължина на тръбопровод, надвишаваща 10 м)","0,02 (за дължина на тръбопровод, надвишаваща 10 м)","0,02 (за дължина на тръбопровод, надвишаваща 10 м)"]
["","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","15","15","15","15","20"]
["Стандартни аксесоари","Installation manual","","","","1","1","1","1","1"]
["","Drain plug","","","","1"]
["Електрозахранване","Фаза","","","","1~","1~","1~","1~","1~"]
["","Честота","","","Хц","50","50","50","50","50"]
["","Напрежение","","","V","220-240","220-240","220-230-240","220-230-240","220-230-240"]
["Забележки","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]