{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXLG-M"]
[]
[]
[]
[]
["","","","","","RXLG25M2V1B","RXLG35M2V1B"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Свръх ниска","м³/мин","30.6","30.6"]
["","","Отопление","Свръх ниска","м³/мин","27.2","27.2"]
["","","","Свръх ниска","cfm","1080","1080"]
["","","Отопление","Свръх ниска","cfm","960","960"]
["Размери","Тяло","","Височина","мм","550","550"]
["","","","Широчина","мм","858","858"]
["","","","Дълбочина","мм","330","330"]
["Тегло","Тяло","","","kg","40","40"]
["Компресор","Type","","","","","Херметично запечатан люлеещ се компресор"]
["Работен диапазон","Охлаждане","околна температура","Мин.","°CDB","-10","-10"]
["","","","Макс.","°CDB","46","46"]
["","Отопление","околна температура","Мин.","°C (влажен термометър)","-25","-25"]
["","","","Макс.","°C (влажен термометър)","18","18"]
["Ниво на звуково налягане","Охлаждане","","Висок","dBA","48","48"]
["","","","Ниско","dBA","44","44"]
["","Отопление","","Висок","dBA","49","49"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","dBA","45","45"]
["Хладилен агент","Тип","","","","R-410A","R-410A"]
["","Зареждане","","","kg","1","1"]
["","Маса","","","tCO2Eq","2.1","2.1"]
["","Потенциал на глобално затопляне","","","","2087.5","2087.5"]
["Тръбни съединения","Дължина на тръбите","Макс.","Външ. у-во - Вътр. у-во","м","20","20"]
["","Допълнително количество хладилен агент","","","кг/м","0,02 (за дължина на тръбопровод, надвишаваща 10 м)","0,02 (за дължина на тръбопровод, надвишаваща 10 м)"]
["","Разлика в нивата","Вътр. у-во - Вътр. у-во","Макс.","м","15","15"]
["Стандартни аксесоари","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["Електрозахранване","Фаза","","","","1~","1~"]
["","Честота","","","Хц","50","50"]
["","Напрежение","","","V","220-240","220-240"]
["Компресор","Тип","","","","Херметично запечатан люлеещ се компресор"]