{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-A8"]
[]
[]
[]
[]
["","","","","","RXM50A5V1B8"]
["Размери","Тяло","","Височина","мм","610"]
["","","","Широчина","мм","923"]
["","","","Дълбочина","мм","367"]
["Тегло","Тяло","","","kg","40"]
["Електромотор на вентилатор","Скорост","Охлаждане","Свръх ниска","RPM","600"]
["Компресор","Тип","","","","Херметично запечатан люлеещ се компресор"]
["Работен диапазон","Охлаждане","околна температура","Мин.","°C (сух термометър)","-10"]
["","","","Макс.","°C (сух термометър)","50 (1), 46 (1)"]
["","Отопление","околна температура","Мин.","°C с влажен термометър","-21 (1), -15 (1)"]
["","","","Макс.","°C с влажен термометър","18"]
["Ниво на звуково налягане","Охлаждане","","Ном.","дБА","48"]
["","Отопление","","Ном.","дБА","49"]
["Хладилен агент","Тип","","","","R-32"]
["","Зареждане","","","kg","0.95"]
["","Маса","","","tCO2Eq","0.65"]
["","Потенциал на глобално затопляне","","","","675"]
["Тръбни съединения","Дължина на тръбите","Макс.","Външ. у-во - Вътр. у-во","м","30"]
["","Допълнително количество хладилен агент","","","кг/м","002 (за дължина на тръбопровод надвишаваща 10 м)"]
["","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","20"]
["Стандартни аксесоари","Installation manual","","","","1"]
["","Drain joint","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","LOT10 Energy Label","","","","1"]
["","Drain cap","","","","3"]
["Електрозахранване","Фаза","","","","1~"]
["","Честота","","","Хц","50"]
["","Напрежение","","","V","220-240"]
["Забележки","","","","","(1) - Вж. отделния чертеж за работен диапазон"]
["","","","","","(2) - Вж. отделния чертеж за електрическите схеми"]
["","","","","","(3) - Съдържа флуорирани парникови газове"]