{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":9,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-N"]
[]
[]
[]
[]
["","","","","","RXM42N2V1B","RXM50N2V1B","RXM60N2V1B","RXM71N2V1B"]
["Размери","Тяло","","Височина","mm","734","734","734","734"]
["","","","Широчина","mm","870","870","870","870"]
["","","","Дълбочина","mm","373","373","373","320"]
["Тегло","Тяло","","","kg","50","50","50","56"]
["Компресор","Type","","","","Херметично запечатан люлеещ се компресор","","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор"]
["Работен диапазон","Охлаждане","околна температура","Мин.","°CDB","-10","-10","-10","-10"]
["","","","Макс.","°CDB","46","46","46","46"]
["","Отопление","околна температура","Мин.","°C с влажен термометър","-15","-15","-15","-15"]
["","","","Макс.","°C с влажен термометър","18","18","18","18"]
["Ниво на звуково налягане","Охлаждане","","Ном.","дБА","48.0","48.0","48.0","47"]
["","Отопление","","Ном.","дБА","48.0","49.0","49.0","48"]
["Хладилен агент","Тип","","","","R-32","R-32","R-32","R-32"]
["","Зареждане","","","kg","1.10","1.15","1.15","1.15"]
["","Маса","","","tCO2Eq","0.75","0.78","0.78","0.78"]
["","Потенциал на глобално затопляне","","","","675","675","675","675.0"]
["Тръбни съединения","Дължина на тръбите","Макс.","Външ. у-во - Вътр. у-во","м","30","30","30","30.0"]
["","Допълнително количество хладилен агент","","","кг/м","0,02 (за дължина на тръбопровод, надвишаваща 10 м)","0,02 (за дължина на тръбопровод, надвишаваща 10 м)","0,02 (за дължина на тръбопровод, надвишаваща 10 м)","0,02 (за дължина на тръбопровод, надвишаваща 10 м)"]
["","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","20","20","20","20.0"]
["Стандартни аксесоари","Installation manual","","","","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1"]
["","Drain cap","","","","3","3","3","3"]
["","Drain plug","","","","1","1","1","1"]
["Електрозахранване","Фаза","","","","1~","1~","1~","1~"]
["","Честота","","","Хц","50","50","50","50"]
["","Напрежение","","","V","220-240","220-240","220-240","220-240"]
["Компресор","Тип","","","","","Херметично запечатан люлеещ се компресор"]